Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Downloads
- CTP1000 Console Cable Pinouts

- Related Topics
- CTP Fast Ethernet and Power Cables

# CTP1000 Console Cable Pinouts

A console is connected to the CTP1002, CTP1004, and CTP1012 devices with a DB-9 crossover cable. The console connections are configured to the following parameters:

- Speed: 9600 bps
- Data bits: 8
- Stop bits: 1
- Flow control: Xon/Xoff
- Parity: none

Table 1 lists console cable pinouts for CTP1000 devices.

Table 1: CTP1000 Series Console Cable Pinouts

CTP DB-9 Pin | Console DB-9 Pin
--- | ---
2 RCV | 3 XMT
3 XMT | 2 RCV
4 DTR | 6 DSR
5 GND | 5 GND
6 DSR | 4 DTR
7 RTS | 8 CTS
8 CTS | 7 RTS
9 RNG | —

#### Published: 2010-05-11