Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Voice Compression Module Overview
- Calculating Resource Usage on Voice Compression Modules Overview

# Configuring Compression Parameters for VComp Bundles (CTPView)

This topic describes how to configure compression options for VComp bundles.

Before you begin:

- Log in to the CTPView software at least at the Net_Admin level.
- Connect the CTPView server to the CTP device for which you want to configure bundles.
- Disable the bundle before you modify the bundle options.

To configure compression parameters for VComp bundles using CTPView:

1. In the side pane, select Bundle > Configuration.
2. Run your mouse over the Display and Select an Existing Bundle bar.
3. In the table of bundles, select the bundle that you want to modify.
4. Under Bundle Options, configure the parameters described in Table 1, and click Click to Submit Bundle AND Port Changes.

Table 1: VComp Bundle Compression Parameter Settings in CTPView

Field | Function | Your Action
--- | --- | ---
Companding | Specifies the pulse-code modulation (PCM) encoding standard used on the port PCM input to the VComp bundle. When a VComp bundle is built with: Analog voice interfaces, this configuration is applied on both the analog voice port and the voice compression module, so there are no compatibility issues. T1/E1 channels, set companding to match the type of companding that is used for the external connecting equipment. Generally, mu-law is used in the US, and a-law is used in Europe and elsewhere. | Select one: Transparent—Applies to T1/E1 ports only. Choose this option to transport lossless data in a VComp bundle (that is, for carrying a CCS signaling D channel). Mu-law—Generally used in the United States. A-law—Generally used in Europe and elsewhere.
Codec | Specifies the level and type of voice compression performed on voice channels. See Calculating Resource Usage on Voice Compression Modules Overview for information about the voice compression module utilization and compression level for each compression type. | Select one: MELP (2.4k) G.729AB (8k) G.728 (16k) G.726 (16k) G.726 (32k) G.711 (64k)
Echo Cancellation | Enables or disables echo cancellation. When this option is enabled, 32 ms of local tail echo cancellation is performed on every bundle channel. | Select one: No Yes
Silence Detection | Enables or disables silence detection. When this option is enabled and silence is detected on the channel, the network bandwidth used for that channel is reduced drastically. This behavior can create significant network bandwidth savings. | Select one: No Yes
Fax/Modem Support | Enables or disables detection of fax and modem tones. When enabled and fax or modem tones are detected on the line, compression is disabled and the channel reverts to PCM. Although enabling this attribute increases the amount of network bandwidth needed for that channel in the bundle for the duration of the fax or modem session, it succeeds in negotiation and transfer of fax and modem data at high speeds. | Select one: No Yes
Tone Relay | When enabled and tones are detected at the local end port, they are transported and regenerated at the remote end. This is an important option particularly for high compression levels, where tones may be distorted if they are compressed. The tone relay types supported are DTMF and MFR1. | Select one: No Yes

## Related Documentation

- Voice Compression Module Overview
- Calculating Resource Usage on Voice Compression Modules Overview

#### Published: 2010-10-27

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out