Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# CTP150 Platform Specifications

Table 1: CTP150 Platform Specifications

Category | Specification
--- | ---
Weight |
Chassis only | 14.5 lb (6.6 kg)
Dimensions |
Chassis only | 1.73 in. (4.4 cm) high 17.24 in. (43.8 cm) wide 14.5 in. (36.8 cm) deep
Environmental Requirements |
Ambient operating temperature | 32 to 104° F (0 to 40° C)
Ambient operating humidity | 5% to 90% (noncondensing)
DC Input | N/A
AC Input |
Power required | 100–240 VAC
AC line frequency | 50–60 Hz
Nominal current (115V amps) | <1.0
Power | 100 W
Space Requirements | 3 ft. (90 cm) behind device or rack. Do not block air vents on the front or back of the device.
Airflow | Fan
Safety Agency Certification | AS/NZS 60950.1-2003 Safety of Information Technology Equipment CAN/CSA-C22.2 No. 60950-1 (2007) Information Technology Equipment - Safety EN 60950-1 (2005) Information Technology Equipment - Safety IEC 60950-1 (2005) Information Technology Equipment - Safety (All country deviations) Low Voltage Directive (2006/95/EC) UL 60950-1 (1st Ed.) Information Technology Equipment - Safety
Electromagnetic Emissions Agency Certification | AS/NZS CISPR 22:2004 BSMI CNS 13438 and NCC C6357 Taiwan Radiated Emissions EMC Directive (89/336/EEC) EN 300 386 V1.3.3 (2005) Telecom Network Equipment - EMC requirements EN 55022 Class A (2006) European Radiated Emissions EN 55024 +A1+A2 (1998) Information Technology Equipment Immunity Characteristics EN-61000-3-2 (2006) Power Line Harmonics (2006) Power Line Harmonics EN-61000-3-3 +A1 +A2 +A3 (1995) Power Line Voltage Fluctuations EN-61000-4-2 +A1 +A2 (1995) Electrostatic Discharge EN-61000-4-3 +A1+A2 (2002) Radiated Immunity EN-61000-4-4 (2004) Electrical Fast Transients EN-61000-4-5 (2006) Surge EN-61000-4-6 (2007) Immunity to Conducted Disturbances ETSI 300-386, Telecommunication Network Equipment; ElectroMagnetic Compatibility (EMC) requirements FCC Part 15 Class A (2007) USA Radiated Emissions IECS-03 Issue 3 Class A VCCI Class A (2007) Japanese Radiated Emissions

#### Published: 2011-01-31

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out