Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# Configuring the Default Bundle Data Protocol on the CTP Device (CTP Menu)

The default bundle data protocol is GRE (47). Before you configure SAToP bundles, you should change the default bundle data protocol to a value other than GRE. Doing so prevents conflict between legacy CTP bundles and SAToP bundles that are using GRE for interoperability.

To configure the default data protocol for bundles from GRE using CTP Menu:

1. From the Main Menu, select 5) Node Operations.
2. Select 3) Configure network settings.
3. Select 6) CTP Bndl Data pkt protocol.

   You are notified that changing this parameter requires a system reboot.

4. Enter a number other than 47 as the protocol for data packets.
5. Reboot the CTP device.

#### Published: 2010-10-21

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out