Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Downloads
- Installing the CTP1000 Platform in Freestanding Mode

- Related Topics
- Before You Install the CTP1000 Platform
- Installing the CTP1000 Platform in a Rack
- Cabling the CTP1000 Platform Overview

# Installing the CTP1000 Platform in Freestanding Mode

When installing the device on a table top or in any other freestanding mode, be sure to leave enough space around the device for adequate ventilation. Position the chassis with easy access to the connections that it needs for power, local communications, and remote communications.

| Warning: At least two people are required to lift the device. Three people are required for the heavier CTP platforms.

| Caution: To prevent electrostatic damage to the device and its components, make sure that persons handling the device wear an antistatic device.

#### Published: 2010-05-11