Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- SAToP Bundle Overview

# Configuring Virtual IP Parameters for SAToP Bundles (CTPView)

The virtual IP parameters allow you to use a separate IP address for each bundle and to use an address that is different from the IP address for the CTP device. If you configure the IP address on the:

- Same subnet as CTP IP address, you do not need a static route on the router.
- Different subnet as CTP IP address, you need a static route on the router.

Before you begin:

- Log in to the CTPView software at least at the Net_Admin level.
- Create a list of the virtual IP addresses that will be associated with the CTP device. To do so, select Node > Maintenance > Configure CTP Device Virtual IPs, and follow the instructions on the pane. You can create up to 56 virtual IP addresses.

  When you submit your new configuration, the CTP device reboots.

- Connect the CTPView server to the CTP device for which you want to configure bundles.
- Disable the bundle before you modify the bundle options.

To configure virtual IP parameters for SAToP bundles using CTPView:

1. In the side pane, select Bundle > Configuration.
2. Run your mouse over the Display and Select an Existing Bundle bar.
3. In the table of bundles, select the bundle that you want to modify.
4. Under Bundle Options, place a check mark in the Advanced Options show check box to display advanced parameters, and configure the parameters described in Table 1.

5. Click Click to Submit Bundle AND Port Changes.

Table 1: SAToP Bundle Virtual IP Parameter Settings in CTPView

Field | Function | Your Action
--- | --- | ---
Use Virtual IP | Specifies whether or not the bundle uses an address that is different from the IP address of the CTP device. The virtual IP address is used in the IP packet’s Origination Address field, and is used for the circuit’s data and OAM flow. | Select one: DISABLED—Circuits created by this bundle use the IP address of the CTP device. ENABLED—Circuits created by this bundle use an address that is different from the CTP device.
Virtual IP [ IPv4 only ] | Specifies the virtual IP address for circuits created by this bundle. | Enter the virtual IP address. At the remote end of the bundle, specify this IP address as the Remote Address of the bundle.

## Related Documentation

- SAToP Bundle Overview

#### Published: 2010-10-21

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out