Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring CLI-Based Mirroring
- Configuring RADIUS-Based Mirroring

# mirror disable

#### Syntax

To disable mirroring for a specified trigger type:

mirror disable triggerType [hex] triggerValue

To disable mirroring for the agent-circuit-id or agent-remote-id trigger types, when the hex variant is used:

mirror disable triggerType hex triggerValue

To disable mirroring for the dhcp-option-82 trigger type:

mirror disable dhcp-option-82 agent-circuit-id triggerValue1 agent-remote-id triggerValue2

To disable mirroring for the dhcp-option-82 trigger type, when the hex variant is used:

mirror disable dhcp-option-82 hex triggerValue

#### Release Information

Command introduced before JunosE Release 7.1.0.
nas-port-id added in JunosE Release 7.1.0.

hex keyword added in JunosE Release 11.1.0.

#### Description

Disables a packet mirroring session that was dynamically configured for a subscriber; uses the trigger information to identify the subscriber's session. There is no no version.

| Note: The hex variant is applicable only for agent-circuit-id, agent-remote-id, and dhcp-option-82 trigger types. If the hex variant is used then the triggerValue must be a hexadecimal number.

#### Options

- triggerType—One of the following RADIUS attributes that was used as the trigger to start the packet mirroring session
  - acct-session-id—Acct-Session-Id, RADIUS attribute [44]
  - agent-circuit-id—Agent Circuit ID, RADIUS attribute [26–1], Vendor ID 3561
  - agent-remote-id—Agent Remote ID, RADIUS attribute [26–2], Vendor ID 3561
  - calling-station-id—Calling-Station-Id, RADIUS attribute [31]
  - dhcp-option-82—DHCP Option 82, RADIUS attribute [26–159], Vendor ID 4874
  - ip-address—Framed-IP-Address, RADIUS attribute [8]; associated with the virtual router where the command is issued, RADIUS VSA [26-1]
  - nas-port-id—NAS-Port-Id, RADIUS attribute [87]
  - username—User-Name, RADIUS attribute [1]; associated with the virtual router where the command is issued, RADIUS VSA [26-1]
- triggerValue—Value of the triggerType (the specified RADIUS attribute) that identifies the subscriber

#### Mode

Privileged Exec

## Related Documentation

- Configuring CLI-Based Mirroring
- Configuring RADIUS-Based Mirroring

#### Published: 2011-09-29

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out