# DSL Forum VSAs Supported for AAA Access and Accounting Messages

Table 45 lists the DSL Forum VSAs supported by JunosE Software in Access-Request, Acct-Start, Acct-Stop, (if Acct-Stop is specified) Interim-Acct, and CoA-Request messages. JunosE Software uses the vendor ID assigned to the DSL Forum (3561, or DE9 in hexadecimal format) by the IANA.

Table 45: DSL Forum (Vendor ID 3561) VSAs Supported in AAA Access and Accounting Messages

Attribute Number | Attribute Name | Access-Request | Acct-Start | Acct-Stop | Interim-Acct | CoA-Request
--- | --- | --- | --- | --- | --- | ---
[26-1] | Agent-Circuit-Id | ✓ | ✓ | ✓ | ✓ | ✓
[26-2] | Agent-Remote-Id | ✓ | ✓ | ✓ | ✓ | ✓
[26-129] | Actual-Data-Rate-Upstream | ✓ | ✓ | ✓ | ✓ | –
[26-130] | Actual-Data-Rate-Downstream | ✓ | ✓ | ✓ | ✓ | –
[26-131] | Minimum-Data-Rate-Upstream | ✓ | ✓ | ✓ | ✓ | –
[26-132] | Minimum-Data-Rate-Downstream | ✓ | ✓ | ✓ | ✓ | –
[26-133] | Attainable-Data-Rate-Upstream | ✓ | ✓ | ✓ | ✓ | –
[26-134] | Attainable-Data-Rate-Downstream | ✓ | ✓ | ✓ | ✓ | –
[26-135] | Maximum-Data-Rate-Upstream | ✓ | ✓ | ✓ | ✓ | –
[26-136] | Maximum-Data-Rate-Downstream | ✓ | ✓ | ✓ | ✓ | –
[26-137] | Minimum-Data-Rate-Upstream-Low-Power | ✓ | ✓ | ✓ | ✓ | –
[26-138] | Minimum-Data-Rate-Downstream-Low-Power | ✓ | ✓ | ✓ | ✓ | –
[26-139] | Maximum-Interleaving-Delay-Upstream | ✓ | ✓ | ✓ | ✓ | –
[26-140] | Actual-Interleaving-Delay-Upstream | ✓ | ✓ | ✓ | ✓ | –
[26-141] | Maximum-Interleaving-Delay-Downstream | ✓ | ✓ | ✓ | ✓ | –
[26-142] | Actual-Interleaving-Delay-Downstream | ✓ | ✓ | ✓ | ✓ | –
[26-144] | Access-Loop-Encapsulation | ✓ | ✓ | ✓ | ✓ | –
[26-254] | IWF-Session | ✓ | ✓ | ✓ | ✓ | –

#### Related Documentation

- Subscriber AAA Access Messages Overview
- Subscriber AAA Accounting Messages Overview
- DSL Forum VSAs in AAA Access and Accounting Messages Overview
- CLI Commands Used to Include DSL Forum VSAs in Access and Accounting Messages
- DSL Forum VSAs