Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Juniper Networks VSAs Supported for Subscriber AAA Access Messages
- Juniper Networks VSAs Supported for Subscriber AAA Accounting Messages
- RADIUS Attributes Supported for CLI AAA Messages
- Juniper Networks VSAs
- radius icr-partition-accounting
- radius ignore
- radius include

# CLI Commands Used to Configure Juniper Networks VSAs

Table 1 lists the Juniper Networks VSAs and the corresponding CLI commands used to modify them. The attributes are listed numerically.

Table 1: CLI Commands Used to Configure Juniper Networks VSAs

Attribute Number | Attribute Name | CLI Command
--- | --- | ---
[26-1] | Virtual-Router | radius ignore virtual-router
[26-10] | Ingress-Policy-Name | radius include ingress-policy-name radius ignore ingress-policy-name
[26-11] | Egress-Policy-Name | radius include egress-policy-name radius ignore egress-policy-name
[26-14] | Service-Category | radius ignore atm-service-category
[26-15] | PCR | radius ignore atm-pcr
[26-16] | SCR | radius ignore atm-scr
[26-17] | MBS | radius ignore atm-mbs
[26-24] | Pppoe-Description | radius include pppoe-description
[26-35] | Acct-Input-Gigapackets | radius include input-gigapkts
[26-36] | Acct-Output-Gigapackets | radius include output-gigapkts
[26-44] | Tunnel-Interface-Id | radius include tunnel-interface-id
[26-45] | Ipv6-Virtual-Router | radius include ipv6-virtual-router
[26-46] | Ipv6-Local-Interface | radius include ipv6-local-interface
[26-47] | Ipv6-Primary-DNS | radius include ipv6-primary-dns
[26-48] | Ipv6-Secondary-DNS | radius include ipv6-secondary-dns
[26-51] | Disconnect-Cause | radius include l2tp-ppp-disconnect-cause
[26-53] | Service-Description | radius include profile-service-description
[26-55] | DHCP-Options | radius include dhcp-options
[26-56] | DHCP-MAC-Address | radius include dhcp-mac-address
[26-57] | DHCP-GI-Address | radius include dhcp-gi-address
[26-62] | MLPPP-Bundle-Name | radius include mlppp-bundle-name
[26-63] | Interface-Desc | radius include interface-description
[26-81] | L2C-Information | radius include access-loop-parameters
[26-92] | L2C-Up-Stream-Data | radius include l2c-upstream-data
[26-93] | L2C-Down-Stream-Data | radius include l2c-downstream-data
[26-129] | Ipv6-NdRa-Prefix | radius include ipv6-nd-ra-prefix
[26-141] | Downstream-Calculated-Qos-Rate | radius include downstream-calculated-qos-rate access-request radius include downstream calculated-qos-rate acct-start radius include downstream-calculated-qos-rate acct-stop
[26-142] | Upstream-Calculated-Qos-Rate | radius include upstream-calculated-qos-rate access-request radius include upstream calculated-qos-rate acct-start radius include upstream-calculated-qos-rate acct-stop
[26-143] | Max-Clients-Per-Interface | radius ignore pppoe-max-session
[26-150] | ICR-Partition-Id | radius include icr-partition-id radius icr-partition-accounting
[26-151] | IPv6-Acct-Input-Octets | radius include ipv6-accounting
[26-152] | IPv6-Acct-Output-Octets | radius include ipv6-accounting
[26-153] | IPv6-Acct-Input-Packets | radius include ipv6-accounting
[26-154] | IPv6-Acct-Output-Packets | radius include ipv6-accounting
[26-155] | IPv6-Acct-Input-Gigawords | radius include ipv6-accounting
[26-156] | IPv6-Acct-Output-Gigawords | radius include ipv6-accounting
[26-159] | DHCP-Option 82 | radius include dhcp-option-82

## Related Documentation

- Juniper Networks VSAs Supported for Subscriber AAA Access Messages
- Juniper Networks VSAs Supported for Subscriber AAA Accounting Messages
- RADIUS Attributes Supported for CLI AAA Messages
- Juniper Networks VSAs
- radius icr-partition-accounting
- radius ignore
- radius include

#### Published: 2011-10-21

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out