Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Guidelines for Deactivating High Availability
- Stateful Line Module Switchover Modes
- Application Support for Stateful Line Module Switchover
- line-card switch
- mode
- show redundancy history
- show redundancy line-card

# Deactivating High Availability

When you disable stateful line module switchover, both the primary and standby line modules are shifted to the online state. Both line module redundancy and stateful switchover of line modules are disabled. If the router uses redundant line modules, after you disable high availability, the router uses line module redundancy mode, which is the default behavior.

To disable high availability support:

1. From Global Configuration mode, launch Redundancy Configuration mode.
   host1(config)#redundancy
2. In Redundancy Configuration mode, disable high availability on the line module pair previously configured for stateful switchover
   host1(config-redundancy)#no mode high availability slot 11 16

In this example, high availability behavior configured for the primary line module that resides in slot 11 and the line secondary module installed in slot 16 is removed.

In this scenario, if slot 11 is in online state and slot 16 is in standby state, a warning message is displayed prompting you to confirm (enter y for yes, n for no) whether you want to proceed with the reloading of the line module in slot 16 and whether you want the primary and secondary modules to removed from the high availability pair. If you enter yes, the line module pair is disabled for stateful switchover after a reload operation is completed on slot 16. If you enter no, the high availability setting continues to be activated on the line module pair.

Alternatively, if the secondary line module in slot 16 has taken over the role of the primary line module in slot 11, and if you disable high availability on the line module pair, a warning message is displayed prompting you to confirm (enter y for yes, n for no) whether you want to proceed with the reloading of both the line modules in slot 16 and slot 11 and whether you want the modules to removed from the high availability pair. If you enter yes, the line module pair is disabled for stateful switchover after a reload operation is completed on slot 16 and slot 11. If you enter no, the high availability setting continues to be activated on the line module pair.

## Related Documentation

- Guidelines for Deactivating High Availability
- Stateful Line Module Switchover Modes
- Application Support for Stateful Line Module Switchover
- line-card switch
- mode
- show redundancy history
- show redundancy line-card

#### Published: 2011-09-20

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out