# Monitoring the Configuration of the RADIUS Dynamic-Request Server

#### Purpose

Display the configuration of the RADIUS dynamic-request server.

#### Action

To display the configuration of the RADIUS dynamic-request server:

    host1#show radius dynamic-request servers

                   RADIUS Request Configuration
                   ----------------------------
                                           Change
                    Udp                      Of
     IP Address     Port   Disconnect   Authorization   Secret
    -------------   ----   ----------   -------------   ------
    192.168.2.3     1700   disabled     disabled        <NULL>
    10.10.120.104   1700   disabled     disabled        mysecret

#### Meaning

Table 66 lists the show radius dynamic-request servers command output fields.

Table 66: show radius dynamic-request servers Output Fields

Field Name | Field Description
--- | ---
IP address | IP address of the RADIUS server
Udp Port | Port on which the router listens for RADIUS server
Disconnect | Status of RADIUS-initiated disconnect feature
Change of Authorization | Status of change of authorization feature
Secret | Secret used to connect to RADIUS server

#### Related Documentation

- show radius servers