Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# line

#### Syntax

line { console lineNumber | vty lineRangeStart [ lineRangeEnd ] }

no line vty lineNumber

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Opens virtual terminal lines or the console line and allows you to configure the lines. By default five vty lines (0–4) are open. The no version removes a vty line or a range of lines from your configuration; users will not be able to run Telnet, SSH, or FTP to lines that you remove. When you remove a vty line, the router removes all lines above that line. For example, no line vty 6 causes the router to remove lines 6 through 29. You cannot remove lines 0 through 4.

| Note: Once lines are open, login is enabled by default. Before users can access the lines, you must configure a password, disable login using the no login command, or configure AAA authentication on the line.

#### Options

- console—Specifies the console line
- vty—Specifies vty lines
- lineNumber—Number of a single line; 0 for the console line
- lineRangeStart—Start of the vty line range; a number from 0–29
- lineRangeEnd—End of the vty line range; a number from 0–29

#### Mode

Global Configuration

#### Published: 2011-09-29

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out