# CLI Commands Used to Configure Juniper Networks VSAs

Table 48 lists the Juniper Networks VSAs and the corresponding CLI commands used to modify them. The attributes are listed numerically.

Table 48: CLI Commands Used to Configure Juniper Networks VSAs

Attribute Number | Attribute Name | CLI Command
--- | --- | ---
[26-1] | Virtual-Router | radius ignore virtual-router
[26-10] | Ingress-Policy-Name | radius include ingress-policy-name radius ignore ingress-policy-name
[26-11] | Egress-Policy-Name | radius include egress-policy-name radius ignore egress-policy-name
[26-14] | Service-Category | radius ignore atm-service-category
[26-15] | PCR | radius ignore atm-pcr
[26-16] | SCR | radius ignore atm-scr
[26-17] | MBS | radius ignore atm-mbs
[26-24] | Pppoe-Description | radius include pppoe-description
[26-35] | Acct-Input-Gigapackets | radius include input-gigapkts
[26-36] | Acct-Output-Gigapackets | radius include output-gigapkts
[26-44] | Tunnel-Interface-Id | radius include tunnel-interface-id
[26-45] | Ipv6-Virtual-Router | radius include ipv6-virtual-router
[26-46] | Ipv6-Local-Interface | radius include ipv6-local-interface
[26-47] | Ipv6-Primary-DNS | radius include ipv6-primary-dns
[26-48] | Ipv6-Secondary-DNS | radius include ipv6-secondary-dns
[26-51] | Disconnect-Cause | radius include l2tp-ppp-disconnect-cause
[26-53] | Service-Description | radius include profile-service-description
[26-55] | DHCP-Options | radius include dhcp-options
[26-56] | DHCP-MAC-Address | radius include dhcp-mac-address
[26-57] | DHCP-GI-Address | radius include dhcp-gi-address
[26-62] | MLPPP-Bundle-Name | radius include mlppp-bundle-name
[26-63] | Interface-Desc | radius include interface-description
[26-81] | L2C-Information | radius include access-loop-parameters
[26-92] | L2C-Up-Stream-Data | radius include l2c-upstream-data
[26-93] | L2C-Down-Stream-Data | radius include l2c-downstream-data
[26-129] | Ipv6-NdRa-Prefix | radius include ipv6-nd-ra-prefix
[26-141] | Downstream-Calculated-Qos-Rate | radius include downstream-calculated-qos-rate access-request radius include downstream calculated-qos-rate acct-start radius include downstream-calculated-qos-rate acct-stop
[26-142] | Upstream-Calculated-Qos-Rate | radius include upstream-calculated-qos-rate access-request radius include upstream calculated-qos-rate acct-start radius include upstream-calculated-qos-rate acct-stop
[26-143] | Max-Clients-Per-Interface | radius ignore pppoe-max-session
[26-150] | ICR-Partition-Id | radius include icr-partition-id radius icr-partition-accounting
[26-151] | IPv6-Acct-Input-Octets | radius include ipv6-accounting
[26-152] | IPv6-Acct-Output-Octets | radius include ipv6-accounting
[26-153] | IPv6-Acct-Input-Packets | radius include ipv6-accounting
[26-154] | IPv6-Acct-Output-Packets | radius include ipv6-accounting
[26-155] | IPv6-Acct-Input-Gigawords | radius include ipv6-accounting
[26-156] | IPv6-Acct-Output-Gigawords | radius include ipv6-accounting
[26-159] | DHCP-Option 82 | radius include dhcp-option-82

#### Related Documentation

- Juniper Networks VSAs Supported for Subscriber AAA Access Messages
- Juniper Networks VSAs Supported for Subscriber AAA Accounting Messages
- RADIUS Attributes Supported for CLI AAA Messages
- Juniper Networks VSAs
- radius icr-partition-accounting
- radius ignore
- radius include