# radius dsl-port-type

#### Syntax

radius dsl-port-type { sdsl | adsl-cap | adsl-dmt | idsl | xdsl | virtual }

no radius dsl-port-type

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets RADIUS attribute 61, NAS-Port-Type, in RADIUS access request packets and accounting start and stop packets for ATM interfaces. The no version restores the default setting, xdsl.

| If the interface (port) is Ethernet, then it sets the attribute to Ethernet and disregards the parameter set with this command. If the interface (port) is DSL, then the attribute can have any value listed in the command and uses the value configured. For subscribers connected over the LAG interface in DHCP standalone authenticate mode, RADIUS calculates the value of the Nas-Port-Type attribute.

#### Options

- sdsl—Symmetric DSL
- adsl-cap—Asymmetric DSL, carrierless amplitude phase modulation
- adsl-dmt—Asymmetric DSL, discrete multitone
- idsl—ISDN DSL
- xdsl—DSL of unspecified type (default)
- virtual—Virtual

#### Mode

Global Configuration