Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Creating Parameter Instances
- Creating a QoS Parameter on an Interface Superset or Interface Set

# qos-parameter

#### Syntax

In Global Configuration, Interface Configuration, QoS Interface Set Configuration, and QoS Interface Superset Configuration modes:

qos-parameter qosParameterInstanceName qosParameterInstanceValue

no qos-parameter

In Profile Configuration mode:

qos-parameter qosParameterInstanceName [ qosParameterInstanceValue |
add qosParameterAddValue [ initial-value qosParameterInitialValue ] ]

no qos-parameter qosParameterInstanceName [ add ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
add and initial-value keywords added in JunosE Release 7.2.0.
Profile Configuration mode added in JunosE Release 7.2.0.

QoS Interface Set Configuration and QoS Interface Superset Configuration modes added in JunosE Release 9.2.0.

#### Description

In Global Configuration mode, creates a QoS parameter instance and assigns a value to the parameter. A global parameter instance is typically used to provide a global default for a parameter value. The no version deletes the parameter instance.

In Interface Configuration mode, creates a parameter instance, assigns a value to the parameter, and attaches the parameter instance to the interface. The no version detaches the parameter instance from the interface.

In Profile Configuration mode, creates a parameter instance command in a profile for use with Service Manager. When the service is activated, the parameter instances are created for the subscriber interface. The no version removes the parameter instance command from the profile.

In QoS Interface Set Configuration mode, creates a parameter instance, assigns a value to the parameter, and attaches the parameter instance to a QoS interface set. The no version detaches the parameter instance from the interface set.

In QoS Interface Superset Configuration mode, creates a parameter instance, assigns a value to the parameter, and attaches the parameter instance to a QoS interface superset. The no version detaches the parameter instance from the interface superset.

#### Options

- qosParameterInstanceName—Name of the QoS parameter instance
- qosParameterInstanceValue—Number of the rate for the parameter instance; the default value is the minimum value defined in the parameter definition
- qosParameterAddValue—Number of the rate that is added to an existing parameter instance
- qosParameterInitialValue—Number of the initial rate of a newly created parameter instance

#### Mode

Global Configuration, Interface Configuration, Profile Configuration, QoS Interface Set Configuration, QoS Interface Superset Configuration

## Related Documentation

- Creating Parameter Instances
- Creating a QoS Parameter on an Interface Superset or Interface Set

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out