# show subscribers

#### Syntax

To display detailed information:

show subscribers [ ipv6 [ ipv6Prefix ] ]
[ domain domainName | icr-partition icrPartitionLocationId |
interface { atm | ethernet | lag } interfaceSpecifier |
port interfaceSpecifier | slot slotNumber | username userName |
virtual-router vrName ] [ filter ]

To display summary information:

show subscribers summary [ domain | icr-partition | interface | port | slot | virtual-router | lag ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
interface, atm, and ethernet keywords added in JunosE Release 7.3.0.
slot keyword and slotNumber variable added in JunosE Release 7.3.0.
icr-partition keyword and icrPartitionLocationId variable added in JunosE Release 10.3.0.
lag keyword added to the show subscribers command in JunosE Release 11.0.0.
lag keyword added to the show subscribers summary command in JunosE Release 12.3.0.

#### Description

Displays the active subscribers on your router.

#### Options

- ipv6—Displays IPv6 subscribers for the domain
- ipv6Prefix—Prefix that defines the IPv6 network that you want to filter
- userName—Username of active subscriber
- domain—Displays active subscribers for the domain
- domainName—Domain name matching usernames of active subscribers
- icr-partition—Displays active subscribers for the ICR partition
- icrPartitionLocationId—A unique identifier for each ICR partition on a chassis. Note that this ID different from the partition ID, which is configured using the ip vrrp vrid icr-partition partitionId command. The partition location ID that you specify here is a combination of the interface within the chassis on which the ICR partition is configured and the VRRP ID, which is system-defined and nonconfigurable.
- interface—Displays active subscribers for the specified interface: atm, ethernet, or lag. In the summary version, displays active subscribers for all ATM, Ethernet, and LAG interfaces
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- port—Displays active subscribers for the port
- slot—Displays active subscribers for the slot
- slotNumber—Number of the chassis slot of the line module in the range 0–2 (ERX310 model), 0–6 (ERX7xx models), 0–13 (ERX14xx models), 0-5 (E120 router), and 0-16 (E320 router)
- virtual-router—Displays active subscribers for the VR
- vrName—Name of the VR to which interfaces of active subscribers are bound
- lag—Displays the consolidated information on active subscribers that are logged in on top of a LAG bundle
- filter—See Filtering show Commands
- summary—Displays the active subscribers for each domain, interface, port, slot, or virtual router

#### Mode

Privileged Exec