# Configuring the Number of ACI-based VLAN Subinterfaces per S-VLAN

You can limit the number of ACI-based VLAN subinterfaces per S-VLAN at the interface level to a configurable value.

To configure the number of ACI-based VLAN subinterfaces per S-VLAN:

- From Interface Configuration mode, configure the number of VLAN subinterfaces.
  host1(config-if)#max aci-svs per-pvs limitvalue

The ACI-based VLAN subinterface limit is visible using the show configuration command.

| Note: Even if you configure the maximum number of ACI-based VLAN subinterfaces per S-VLAN on a VLAN or an S-VLAN subinterface using the max aci-svs per-pvs limitvalue command, the setting is saved on the VLAN major interface. This behavior is expected and you can verify the configured value from the output of the show configuration interface command.

#### Related Documentation

- ACI-based VLAN Subinterfaces per S-VLAN Overview
- max aci-svs per-pvs