# CLI Commands Used to Modify RADIUS Attributes

You can configure the RADIUS Internet Engineering Task Force (IETF) attributes and the Juniper Networks vendor-specific attributes using CLI commands.

For many attributes, you can configure the router to include the attribute in RADIUS messages.

You can also configure the router to ignore many attributes that it receives in Access-Accept messages.

For a complete list of RADIUS attributes supported by JunosE Software, see RADIUS IETF Attributes.

#### Related Documentation

- CLI Commands Used to Configure RADIUS IETF Attributes
- CLI Commands Used to Configure Juniper Networks VSAs
- CLI Commands Used to Include ANCP-Related Juniper Networks VSAs in Access and Accounting Messages
- CLI Commands Used to Include DSL Forum VSAs in Access and Accounting Messages
- CLI Commands Used to Include or Exclude Attributes in RADIUS Messages
- CLI Commands Used to Ignore Attributes when Receiving Access-Accept Messages