Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Subscriber AAA Access Messages Overview
- Subscriber AAA Accounting Messages Overview
- RADIUS IETF Attributes
- Juniper Networks VSAs
- Monitoring Included RADIUS Attributes
- radius include

# CLI Commands Used to Include or Exclude Attributes in RADIUS Messages

You can use the radius include command to enable or disable the inclusion of RADIUS attributes in Acct-on, Acct-off, Access-Request, Acct-Start, and Acct-Stop messages.

Table 1 lists the RADIUS attributes that can be included or excluded in RADIUS messages using the radius include command and the RADIUS messages in which the attributes are supported.

Table 1: RADIUS Attributes Included in Corresponding RADIUS Messages

Attribute Number | Attribute Name | Access-Request | Acct-on | Acct-off | Acct-Start | Acct-Stop
--- | --- | --- | --- | --- | --- | ---
[5] | NAS-Port | ✓ | – | – | ✓ | ✓
[8] | Framed-IP-Address | ✓ | – | – | ✓ | ✓
[9] | Framed-IP-Netmask | – | – | – | ✓ | ✓
[13] | Framed-Compression | – | – | – | ✓ | ✓
[22] | Framed-Route | – | – | – | ✓ | ✓
[25] | Class | – | – | – | ✓ | ✓
[26-10] | Ingress-Policy-Name | – | – | – | ✓ | ✓
[26-11] | Egress-Policy-Name | – | – | – | ✓ | ✓
[26-24] | Pppoe-Description | ✓ | – | – | ✓ | ✓
[26-35] | Acct-Input-Gigapackets | – | – | – | – | ✓
[26-43] | Acct-Output-Gigapackets | – | – | – | – | ✓
[26-44] | Tunnel-Interface-ID | ✓ | – | – | ✓ | ✓
[26-45] | Ipv6-Virtual-Router | – | – | – | – | ✓
[26-46] | Ipv6-Local-Interface | – | – | – | – | ✓
[26-47] | Ipv6-Primary-DNS | – | – | – | – | ✓
[26-48] | Ipv6-Secondary-DNS | – | – | – | – | ✓
[26-51] | Disconnect-Cause | – | – | – | – | ✓
[26-53] | Service-Description | ✓ | – | – | ✓ | ✓
[26-55] | DHCP-Options | ✓ | – | – | ✓ | ✓
[26-56] | DHCP-MAC-Address | ✓ | – | – | ✓ | ✓
[26-57] | DHCP-GI-Address | ✓ | – | – | ✓ | ✓
[26-62] | MLPPP-Bundle-Name | ✓ | – | – | ✓ | ✓
[26-63] | Interface-Description | ✓ | – | – | ✓ | ✓
[26-81] | L2c-Information | ✓ | – | – | – | –
[26-92] | L2C-Up-Stream-Data | ✓ | – | – | ✓ | ✓
[26-93] | L2C-Down-Stream-Data | ✓ | – | – | ✓ | ✓
[26-110] | Acc-Loop-Cir-Id | ✓ | – | – | ✓ | ✓
[26-111] | Acc-Aggr-Cir-Id-Bin | ✓ | – | – | ✓ | ✓
[26-112] | Acc-Aggr-Cir-Id-Asc | ✓ | – | – | ✓ | ✓
[26-113] | Act-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-114] | Act-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-115] | Min-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-116] | Min-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-117] | Att-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-118] | Att-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-119] | Max-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-120] | Max-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-121] | Min-LP-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-122] | Min-LP-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-123] | Max-Interlv-Delay-Up | ✓ | – | – | ✓ | ✓
[26-124] | Act-Interlv-Delay-Up | ✓ | – | – | ✓ | ✓
[26-125] | Max-Interlv-Delay-Dn | ✓ | – | – | ✓ | ✓
[26-126] | Act-Interlv-Delay-Dn | ✓ | – | – | ✓ | ✓
[26-127] | DSL-Line-State | ✓ | – | – | ✓ | ✓
[26-128] | DSL-Type | ✓ | – | – | ✓ | ✓
[26-129] | Ipv6-NdRa-Prefix | – | – | – | – | ✓
[26-141] | Downstream-Calculated-Qos | ✓ | – | – | ✓ | ✓
[26-142] | Upstream-Calculated-Qos-Rate | ✓ | – | – | ✓ | ✓
[26-150] | ICR-Partition-Id | ✓ | – | – | ✓ | ✓
[26-159] | DHCP-Option 82 | ✓ | – | – | ✓ | ✓
[30] | Called-Station-Id | ✓ | – | – | ✓ | ✓
[31] | Calling-Station-Id | ✓ | – | – | ✓ | ✓
[32] | NAS-Identifier | ✓ | ✓ | ✓ | ✓ | ✓
[41] | Acct-Delay-Time | – | ✓ | ✓ | – | –
[44] | Acct-Session-Id | ✓ | ✓ | ✓ | – | –
[45] | Acct-Authentic | – | ✓ | ✓ | – | –
[49] | Acct-Terminate-Cause | – | – | ✓ | – | –
[50] | Acct-Multi-Session-Id | ✓ | – | – | ✓ | ✓
[51] | Acct-Link-Count | – | – | – | ✓ | ✓
[52] | Acct-Input-Gigawords | – | – | – | – | ✓
[53] | Acct-Output-Gigawords | – | – | – | – | ✓
[55] | Event-Timestamp | – | ✓ | ✓ | ✓ | ✓
[61] | NAS-Port-Type | ✓ | – | – | ✓ | ✓
[64] | Tunnel-Type | ✓ | – | – | ✓ | ✓
[65] | Tunnel-Medium-Type | ✓ | – | – | ✓ | ✓
[66] | Tunnel-Client-Endpoint | ✓ | – | – | ✓ | ✓
[67] | Tunnel-Server-Endpoint | ✓ | – | – | ✓ | ✓
[68] | Acct-Tunnel-Connection | ✓ | – | – | ✓ | ✓
[77] | Connect-Info | ✓ | – | – | ✓ | ✓
[82] | Tunnel-Assignment-Id | – | – | – | ✓ | ✓
[83] | Tunnel-Preference | – | – | – | ✓ | ✓
[87] | NAS-Port-Id | ✓ | – | – | ✓ | ✓
[90] | Tunnel-Client-Auth-Id | ✓ | – | – | ✓ | ✓
[91] | Tunnel-Server-Auth-Id | ✓ | – | – | ✓ | ✓
[96] | Framed-Interface-Id | ✓ | – | – | ✓ | ✓
[97] | Framed-Ipv6-Prefix | ✓ | – | – | ✓ | ✓
[99] | Framed-Ipv6-Route | – | – | – | – | ✓
[100] | Framed-IPv6-Pool | – | – | – | – | ✓
[123] | Delegated-IPv6-Prefix | – | – | – | – | ✓
[188] | Ascend-Num-In-Multilink | ✓ | – | – | ✓ | ✓
| All Tunnel-Server-Attributes | ✓ | – | – | ✓ | ✓
| All Ipv6-Accounting Attributes | – | – | – | – | ✓

## Related Documentation

- Subscriber AAA Access Messages Overview
- Subscriber AAA Accounting Messages Overview
- RADIUS IETF Attributes
- Juniper Networks VSAs
- Monitoring Included RADIUS Attributes
- radius include

#### Published: 2011-10-19

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out