Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Monitoring SNMP Secure Packet Mirroring Traps

# snmp-server host

#### Syntax

To specify the SNMP version, community, UDP port, trap category and trap severity:

snmp-server host ipAddress [ version ver ] securityString [ udp-port port ]
[ trapCategory ]* [ trapFilters trapFilter ]

no snmp-server host ipAddress

To specify the ping timeout and trap queue:

snmp-server host ipAddress pingTimeOut timeOutValue
[ trapQueue { drainRate queueDrainRate | full queueFull |
size queueSize }
[ drainRate queueDrainRate | full queueFull | size queueSize ]*]

snmp-server host ipAddress trapQueue
{ drainRate queueDrainRate | full queueFull | size queueSize }
[ drainRate queueDrainRate | full queueFull | size queueSize ]*
[ pingTimeOut timeOutValue ]

no snmp-server host ipAddress { pingTimeOut | trapQueue { drainRate | full | size } }

#### Release Information

Command introduced before JunosE Release 7.1.0.
ip keyword added in JunosE Release 7.1.0.
packetMirror keyword added in JunosE Release 7.2.0.

#### Description

Configures one or more hosts to receive an SNMP trap. The no version removes the specified host from the list of recipients.

#### Options

- ipAddress—IP address of the SNMP trap recipient
- ver—SNMP protocol version for traps sent to host; one of the following values: v1, v2c, or v3
- securityString—SNMP community string
- port—UDP port number of SNMP trap recipient
- trapCategory—SNMP trap category
  - addrPool—Local address pool traps
  - atmPing—E Series router proprietary ATM ping traps
  - bfdmib—BFD MIB traps
  - bgp—BGP state change traps
  - bulkstats—Bulkstats file full and nearly full traps
  - cliSecurityAlert—Security alerts traps
  - dosProtectionPlatform—DoS protection platform traps
  - dvmrp—DVMRP traps
  - dvmrpUni—E Series router proprietary DVMRP traps
  - environment—Power/temperature/fan traps
  - fileXfer—File transfer status change traps
  - inventory—Router inventory/status traps
  - ip—Internet Protocol traps
  - ldp—LDP traps
  - link—SNMP linkUp/linkDown traps
  - log—System log capacity traps
  - mobileIpv4—Mobile IPv4 traps
  - mplste—Mplste traps
  - mrouter—Mrouter traps
  - packetMirror—Secure packet mirroring traps; visible only if packet mirroring is enabled
  - ospf—OSPF traps
  - ping—Ping operation traps (in disman remops MIB)
  - radius—RADIUS traps
  - snmp—SNMP coldstart, warmstart, link, authenticationFailure traps
  - traceroute—Traceroute operation traps (in disman remops MIB)
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- trapFilter—Minimum severity level for filtering traps sent to this host
  - alert—Severity level 1
  - critical—Severity level 2
  - debug—Severity level 7
  - emergency—Severity level 0
  - error—Severity level 3
  - informational—Severity level 6
  - notice—Severity level 5
  - warning—Severity level 4
- timeOutValue—Ping timeout in minutes, in the range 1–90; default value is 1
- trapQueue—Configures the SNMP trap queue for traps sent to this host
- queueDrainRate—Maximum number of traps per second to be sent to the host, in the range 0–2147483647; default value is 0. By default, there is no limit on the number of traps sent per second to the host.
- queueFull—Method used to drop traps when the trap queue is full
  - dropFirstIn—Drops the oldest trap in the queue
  - dropLastIn—Drops the most recent trap added to the queue
- queueSize—Maximum number of traps to be kept in the trap queue, in the range 32–214748364; default value is 32

#### Mode

Global Configuration

## Related Documentation

- Monitoring SNMP Secure Packet Mirroring Traps

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out