# Configuration Examples

To configure a T3 interface, start at the Global Configuration mode, and issue the following commands:

host1(config)#controller t3 0/1 host1(config-controll)#no shutdwon host1(config-controll)#framing c-bit host1(config-controll)#clock source internal module host1(config-controll)#cablelength 220 host1#exit

To configure an E3 interface, use the controller e3 command in place of the controller t3 command.

To configure HDLC channels on a T3 serial interface, issue the following commands:

host1(config)#controller t3 10/0 host1(config-controll)#exit host1(config)#interface serial 10/0 host1(config-subif)#encapsulation ppp host1(config-subif)#ip address 192.32.10.2 255.255.255.0

To configure fractional T3 on an interface, issue the following commands:

host1(config)#controller t3 10/0 host1(config-controll)#dsu mode 0 host1(config-controll)#dsu bandwidth 10000 host1(config-controll)#scramble