Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Parameter Instances for QoS Clients Overview
- For information about creating QoS parameter instances for Service Manager, see JunosE Broadband Access Configuration Guide
- atm-vp qos-parameter
- atm vp-tunnel
- encapsulation vlan
- interface
- qos-parameter
- svlan id
- svlan qos-parameter

# Creating Parameter Instances

You can create QoS parameter instances globally, for an interface, or for a subinterface.

Tasks to create parameter instances are:

## Creating a Global Parameter Instance

To create a global parameter instance:

- Create a parameter instance in Global Configuration mode.
  host1(config)#qos-parameter max-subscriber-bandwidth 6000000

## Creating a Parameter Instance for an Interface

To create a parameter instance for an interface:

1. Specify an interface.
   host1(config)#interface atm 11/0.1 host1(config)#interface gigabitEthernet 2/0
2. Specify the parameter name and the value.
   host1(config-subif)#qos-parameter max-subscriber-bandwidth 6000000

## Creating a Parameter Instance for an ATM VP

Use this procedure to attach a parameter instance to a VP on the interface. Optionally, use the qos-profile keyword to attach a parameter instance to a QoS profile.

To create a parameter instance for an ATM VP:

1. Configure the ATM VP.
   host1(config)#interface atm 2/0 host1(config-if)#atm vp-tunnel 4
2. Do either of the following:
   - Attach the parameter instance to an ATM VP on the interface.
     host1(config-if)#atm-vp 4 qos-parameter max-subscriber-bandwidth 375000
   - Attach the parameter instance and associate with the QoS profile.
     host1(config-if)#atm-vp 4 qos-profile video qos-parameter max-subscriber-bandwidth 375000

## Creating a Parameter Instance for an S-VLAN

Use this procedure to attach a parameter instance to a specified S-VLAN ID on the interface. Optionally, use the qos-profile keyword to attach a parameter instance to a QoS profile.

To create a parameter instance for an S-VLAN:

1. Specify the Ethernet interface and create the VLAN.
   host1(config)#interface gigabitEthernet 3/0 host1(config-if)#encapsulation vlan host1(config-if)#interface gigabitEthernet 3/0.1
2. Specify the S-VLAN ID.
   host1(config-if)#svlan id 1 202
3. Attach the parameter instance to an S-VLAN ID on the interface.
   host1(config-if)#svlan 202 qos-parameter max-subscriber-bandwidth 6000000

## Related Documentation

- Parameter Instances for QoS Clients Overview
- For information about creating QoS parameter instances for Service Manager, see JunosE Broadband Access Configuration Guide
- atm-vp qos-parameter
- atm vp-tunnel
- encapsulation vlan
- interface
- qos-parameter
- svlan id
- svlan qos-parameter

#### Published: 2011-09-27

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out