# Configuring Proxy Neighbor Advertisements

Much like proxy ARP, proxy Neighbor Discovery is a means by which one interface responds to a Neighbor Discovery query on behalf of another interface.

To configure proxy Neighbor Discovery:

1. Access an IPv6 interface.
   host1(config)#interface fastEthernet 0/0 host1(config-if)#
2. Enable Neighbor Discovery on the current interface.
   host1(config)#ipv6 nd

   | Note: This command is redundant when configuring Neighbor Discovery over Ethernet, because neighbor solicitations and advertisements are automatically sent on Ethernet interfaces.

3. Enable IPv6 neighbor proxy.
   host1(config-if)#ipv6 nd proxy

#### Related Documentation

- Understanding Neighbor Discovery
- Configuring Neighbor Discovery
- Monitoring Neighbor Discovery
- ipv6 nd proxy