# CLI Commands Used to Ignore Attributes when Receiving Access-Accept Messages

You can use the radius ignore command to configure the router to ignore or accept a RADIUS attribute from the received Access-Accept messages.

The following attributes can be ignored or accepted using the radius ignore command:

- atm-mbs
- atm-pcr
- atm-scr
- atm-service-category
- egress-policy-name
- framed-ip-netmask
- ingress-policy-name
- pppoe-max-session
- virtual-router

#### Related Documentation

- Subscriber AAA Access Messages Overview
- Monitoring Ignored RADIUS Attributes
- radius ignore