Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- rate-limit-profile

# Setting a One-Rate Rate-Limit Profile

You can use the rate-limit-profile one-rate command to create a rate-limit profile and enter Rate Limit Profile Configuration mode, from which you can configure attributes for the rate-limit profile. See Unresolved xref.

| Note: The JunosE Software includes the layer 2 headers in the calculations it uses to enforce the rates that you specify in rate-limit profiles.

Use one of the ip, ipv6, l2tp, or mpls keywords in front of the command to specify the type of rate-limit profile you want to create or modify. If you do not include one of the keywords, the router creates an IP rate-limit profile by default.

For hierarchical rate limits, do not specify the interface type, but add the hierarchical keyword at the end. The color-aware keyword is only supported on hierarchical rate limits.

If you do not include a one-rate or two-rate keyword, the default is a two-rate rate-limit profile. If you enter a rate-limit-profile command with the one-rate keyword and then type exit, the router creates a rate-limit profile with the default values listed in Table 1.

Table 1: One-Rate Rate-Limit-Profile Defaults

Policy Attribute | Default Value
--- | ---
type | one-rate
committed-rate | 0
committed-burst | 8192
excess-burst | 0
committed-action | transmit
conformed-action | transmit
exceeded-action | drop
mask (IP and IPv6 rate-limit profiles) | 255
exp-mask (MPLS rate-limit profiles) | 7

| Note: We recommend that you do not configure a committed or peak burst size smaller than the MTU of the interface. Doing so causes large packets to be dropped even when they are transmitted at a very low rate.

- Issue the ip rate-limit-profile command in Global Configuration mode:
  host1(config)#ip rate-limit-profile tcpFriendly10Mb one-rate

  | Note: Commands that you issue in Rate Limit Profile Configuration mode do not take effect until you exit from that mode.

## Related Documentation

- rate-limit-profile

#### Published: 2011-10-14

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out