# Monitoring MPLS Explicit Paths

#### Purpose

Display MPLS explicit paths.

#### Action

To display information about all MPLS explicit paths:

    host1:pe2#show mpls explicit-paths
      path name/identifier rx1-path enabled
        1: next-address 70.70.70.2
        2: next-address 30.30.30.1
      not referenced by any options
      path name/identifier rx1-path2 enabled
        1: next-address 60.60.60.2
        2: next-address 40.40.40.1
      not referenced by any options

To display information about the MPLS explicit path named rx1-path2:

    host1:pe2#show mpls explicit-paths name rx1-path2
      path name/identifier rx1-path2 enabled
        1: next-address 60.60.60.2
        2: next-address 40.40.40.1
      not referenced by any options

#### Meaning

Table 73 lists the show mpls explicit-paths command output fields.

Table 73: show mpls explicit-paths Output Fields

Field Name | Field Description
--- | ---
path name/identifier | Name or identifier of explicit path and status, enabled or disabled, followed by list of path links and the IP address for each link’s next address

#### Related Documentation

- show mpls explicit-paths