# Index

A B C D E F G H I J K L M N O P Q R S T U W X

A

> AAA
>   and Mobile IP home agent
> access lists, BGP
> access lists, IP
>   monitoring
>   redirecting traffic with null interface instead
>   redistributing access routes
>   redistributing access-internal routes
>   redistributing static routes
> access-list command 1, 2, 3
> adjustment-factor command
> aggregation flow caches 1
>   configuring
> ANCP (Access Node Control Protocol)
>   adjusting downstream rates
>   monitoring
>   overview
> ANCP commands
>   clear l2c neighbor
>   id
>   l2c
>   l2c end-user-id
>   l2c ip listen
>   l2c ip oif
>   l2c line-configuration
>   l2c max-branches
>   l2c peer-attachment-id
>   max-branches
>   neighbor
>   qos-adaptive-mode
>   session-timeout
> AS-path attribute
> authentication
>   Mobile IP home agent
> authentication commands
>   authentication 1, 2

B

> baseline commands
>   baseline ip
>   baseline ip mobile home-agent
>   baseline ip tunnel-reassembly
> baseline, setting
>   Mobile IP home agent
>   tunnel reassembly
> BFD (Bidirectional Forwarding Detection)
>   BGP peer reachability detection
>   license
>   liveness detection
>   liveness detection interval, negotiating the
>   transmit interval, negotiating the
> BFD commands
>   clear bfd session
>   clear ipv6 bfd session
>   show license bfd
> BGP (Border Gateway Protocol)
>   BFD
>   clearing IP routing table
>   reinstalling routes in IP routing table
>   well-known communities
> Bidirectional Forwarding Detection. See BFD

C

> cache flow, IP
>   monitoring 1, 2
> certificate revocation list. See CRL
> checksum computation 1, 2
> clear commands
>   clear ip mobile binding
>   clear l2c neighbor
> clear ip commands
>   clear ip prefix-list 1, 2
>   clear ip prefix-tree
>   clear ip routes
> clearing L2C neighbors
> communities, BGP
> community lists, BGP
> conventions
>   notice icons
>   text and syntax
> CRL (certificate revocation list) 1
>   checking
>   viewing
> customer support 1
>   contacting JTAC

D

> dead peer detection. See DPD
> default-information originate command
> destination profiles
>   configuring
>   monitoring 1, 2
> destruct timeout period for single-shot tunnels
> digital certificates
>   authenticating the peer
>   base64
>   CA hierarchy
>   certificate chains
>   checking CRLs
>   configuring
>   file extensions
>   generating private/public key pairs
>   monitoring
>   obtaining a public key certificate
>   obtaining a root CA certificate
>   obtaining public keys without 1, 2
>   offline configuration
>   offline enrollment
>   online configuration
>   online enrollment
>   overview
>   signature authentication
>   standards
>   viewing 1, 2, 3, 4
>   X.509v3
> documentation set
>   comments on
> DPD (dead peer detection)
> DVMRP (Distance Vector Multicast Routing Protocol)
>   reassembly of tunnel packets
>   tunnels
> dvmrp destination profile command
> DVMRP with IPSec
>   how it works
>   setting up secure connection
> dynamic IP tunnels
>   configuring
>   monitoring
>   overview
> dynamic tunnels

E

> enable commands
>   enable ipsec-transport
> enable ipsec-transport command
> endpoints, tunnel

F

> filter lists, BGP
> filtering
>   AS paths
>   network prefixes
>   undesirable traffic
> flow statistics commands
>   cache entries
>   cache timeout
>   enabled
>   export destination
>   export source 1, 2
>   ip flow-aggregation cache
>   mask destination
> FQDN (fully qualified domain name) 1, 2, 3
>   aggressive mode
>   user@fqdn format
>   with digital certificates
>   with preshared keys
> fully qualified domain name. See FQDN

G

> GRE (Generic Routing Encapsulation)
>   reassembly of tunnel packets
>   tunnels
> gre destination profile command
> GRE with IPSec
>   how it works
>   setting up secure connection

H

> home agent, Mobile IP. See Mobile IP home agent

I

> idle timeout period for single-shot tunnels
> IKE (Internet Key Exchange)
>   aggressive mode characteristics
>   aggressive mode negotiations
>   authentication without digital certificates 1, 2
>   initiator proposals and policy rules
>   main mode characteristics
>   overview
>   SA negotiation
>   using digital certificates
> IKE commands 1
>   ike local-identity
>   ike peer-identity
> IKE message notification type
> IKE policies 1
>   authentication mode
>   Diffie-Hellman group
>   encryption algorithms
>     3DES
>     DES
>   hash function
>     MD5
>     SHA-1
>   IPSec tunnels
>   lifetime
>   priority
> instance, route map
> interface commands
>   interface null
>   interface tunnel 1, 2
>     ipsec-transport keyword
> interfaces
>   NAT, marking
> internet community, BGP
> Internet Key Exchange. See IKE
> invalid cookies, IPSec
> IP
>   managing the routing table
> IP addresses
>   prefix lists
>   prefix trees
> ip commands
>   ip as-path access-list
>   ip bgp-community new-format
>   ip community-list
>   ip prefix-list 1, 2
>   ip prefix-tree 1, 2, 3
>   ip refresh-route
>   ip route
>   ip tunnel reassembly
> IP flow
>   export
>   sampling
> IP fragmentation
>   reassembling for tunnel packets
> ip mobile commands 1, See also show ip mobile commands
>   ip mobile home-agent
>   ip mobile host
>   ip mobile profile
>   ip mobile secure foreign-agent
>   ip mobile secure host
> ip nat commands 1, See also show ip nat commands
>   address
>   ip nat
>   ip nat inside source list
>   ip nat inside source static
>   ip nat outside source list
>   ip nat outside source static
>   ip nat pool
>   ip nat translation
>   ip nat translation max-entries
> IP reassembly of tunnel packets 1
>   configuring
>   monitoring
> IP security policies
> IP tunnels 1, 2
>   configuring
>   monitoring 1, 2
> IP-in-IP tunnels 1, 2
> IPSec (IP Security) 1, 2, See also L2TP with IPSec
>   AH
>   AH processing
>   concepts
>   configuration
>     examples
>     tasks
>   configuring
>     IKE policy
>     IPSec parameters
>     tunnels
>   digital certificates
>   encapsulation modes
>   encapsulation protocols
>   ESP
>   ESP processing
>   invalid cookies
>   L2TP with IPSec 1, 2
>   license
>   monitoring
>   overview
>   packet encapsulation
>   protocol stack
>   reassembly of tunnel packets
>   remote access 1, 2
>   secure IP interfaces
>   security parameters
>   security parameters per policy type
>   tunnel destination endpoint
>   tunnel failover 1, 2
>   tunnel source endpoint
> IPSec CA identity commands
>   crl
>   enrollment retry-limit
>   enrollment retry-period
>   enrollment url
>   ipsec ca identity
>   issuer-identifier
>   root proxy url
> ipsec certificate commands
>   ipsec certificate-database refresh
>   ipsec certificate-request generate
> ipsec commands 1, See also show ipsec commands
>   ipsec ca authenticate
>   ipsec ca enroll
>   ipsec ca identity
>   ipsec clear
>   ipsec crl 1, 2
>   ipsec identity
>   ipsec ike-policy-rule
>   ipsec isakmp-policy-rule
>   ipsec key generate 1, 2, 3
>   ipsec key manual pre-share
>   ipsec key pubkey-chain rsa
>   ipsec key zeroize 1, 2
>   ipsec lifetime
>   ipsec local-endpoint
>   ipsec option dpd
>   ipsec option nat-t
>   ipsec option tx-invalid-cookie
>   ipsec transform-set
>   key
>   masked-key
> IPSec identity commands
>   common-name
>   country
>   domain-name
>   ipsec identity
>   organization
> IPSec IKE policy commands
>   aggressive-mode 1, 2
>   authentication 1, 2, 3, 4
>   encryption
>   group
>   hash
>   ip address virtual-router
>   ipsec ike-policy-rule 1, 2, 3
>   ipsec isakmp-policy-rule 1, 2
>   lifetime
> IPSec security parameters
>   in relation to IPSec interface
>   inbound SAs 1, 2
>   lifetime
>   lifetime for user SAs
>   manual versus signaled
>   negotiating transforms
>   operational VR
>   outbound SAs 1, 2
>   per IPSec policy type
>   perfect forward secrecy (PFS) 1, 2
>   transform combinations supported
>   transform sets 1, 2
>   transforms supported
>   transport VR 1, 2
> IPSec transport local profile commands
>   pre-share
>   pre-share-masked
> IPSec transport profile commands 1, See also show ipsec transport commands
>   application
>   ipsec transport profile
>   lifetime
>   local ip address
>   pfs group
>   transform-set
> IPSec tunnel profile commands
>   domain-suffix
>   extended-authentication
>   ike local-identity
>   ike peer-identity
>   ip profile
>   ipsec tunnel profile
>   lifetime
>   local ip address
>   local ip identity
>   local ip network
>   max-interfaces
>   peer ip identity
>   pfs group
>   transform
>   tunnel mtu
> IPSec tunnel profiles
> IPv6
>   license
>   monitoring 1, 2

J

> J-Flow commands
>   clear ip flow stats
>   ip flow statistics
>   ip flow-cache entries
>   ip flow-cache timeout active
>   ip flow-cache timeout inactive
>   ip flow-export
>   ip flow-sampling-mode packet-interval
>   ip route-cache flow sampled
> J-Flow statistics, clearing

K

> keepalive messages, NAT-T
> key-string command
> keys, public
>   displaying on router
>   format of
>   obtaining without digital certificates 1, 2

L

> L2C (Layer 2 Control) See ANCP (Access Node Control Protocol)
> L2F, reassembly of tunnel packets
> L2TP (Layer 2 Tunneling Protocol)
>   reassembly of tunnel packets
> l2tp commands
>   l2tp destination profile 1, 2
>   l2tp ignore-receive-data-sequencing
> L2TP with IPSec 1, 2
>   client software supported
>   compatibility
>   configuring
>     client PC
>     E Series router 1, 2
>     IPSec transport profiles
>     L2TP destination profiles 1, 2
>     single-shot tunnels
>   control and data frames
>   group preshared key
>   how it works
>   LNS change of port
>   monitoring
>   NAT interactions
>   overview 1, 2
>   references
>   requirements
>   setting up secure connection
>   troubleshooting
>   tunnel creation
>   with PPP
> license commands
>   license ipsec-tunnels
>   license mobile-ip home-agent
>   license nat
> lifetime, IPSec 1, 2
> limiting translation entries
> local-as community, BGP
> loopback interfaces 1, 2

M

> manual IPSec interfaces
> manuals
>   comments on
> map tag, route map
> match commands 1
>   and route maps
>   match as-paths
>   match community
>   match distance
>   match extcommunity 1, 2
>   match ip address 1, 2, 3, 4, 5
>   match ip next-hop 1, 2, 3, 4, 5
>   match level
>   match metric
>   match metric-type
>   match policy-list
>   match route-type
>   match tag
>   match-set summary prefix-tree 1, 2, 3
> max-interfaces command
> Mobile IP home agent 1, See also ip mobile commands
>   AAA
>   agent discovery
>   authentication
>   configuration prerequisites
>   configuring
>   home address assignment
>   licensing 1, 2, 3
>   monitoring
>   overview
>   platform considerations
>   references
>   registration
>   routing and forwarding
>   security associations
>     for foreign agents
>     for mobile nodes
>   subscriber management
> MTU (maximum transmission unit)
>   IP tunnels

N

> NAT (Network Address Translation)
>   access list rules, creating
>   address pools, defining
>   address translation
>     dynamic
>     inside source
>     outside source
>     static
>   bidirectional
>   configuration examples
>   configuration types
>   configuring
>   dynamic address translation, defining
>   dynamic inside source translation, creating
>   dynamic outside source translation, creating
>   interfaces, specifying inside and outside
>   license
>   monitoring
>   NAT-T
>   overview
>   passthrough mode
>   references
>   static address translation, defining
>   terms 1
>     inside global address
>     inside local address
>     outside global address
>     outside local address
>   timeouts, defining
>   translation entries, limiting
>   translation rules, defining
>   translations, clearing
> NAT-T (Network Address Translation Traversal)
>   configuring
>   ipsec option nat-t command
>   keepalive messages
>   overview
>   show ike sa command
>   show ipsec ike-sa command
>   show ipsec option command
>   tasks
>   UDP encapsulation
>   UDP statistics
> neighbor commands
>   neighbor distribute-list
>   neighbor filter-list 1, 2
>   neighbor prefix-list
>   neighbor prefix-tree
>   neighbor send-community
> Network Address Translation Traversal. See NAT-T
> Network Address Translation. See NAT
> network prefixes, filtering
> next-hop routers
>   setting or redistributing routes for
>   setting/redistributing routes for 1, 2
> no-advertise community, BGP
> no-export community, BGP
> no-export-subconfed community, BGP
> notice icons
> null interface

O

> OSPF (Open Shortest Path First)
>   clearing IP routing table
>   reinstalling routes in IP routing table

P

> peer public keys
>   displaying on router
>   obtaining without digital certificates 1, 2
> perfect forward secrecy
> policy list
>   monitoring
> prefix lists
> prefix trees
> prefixes
>   filtering network
> preventing recursive tunnels
> profile commands
>   profile
> public keys
>   displaying on router
>   format of
>   obtaining without digital certificates 1, 2

Q

> qos-adaptive-mode command

R

> recursive tunnels, preventing
> redistribute command
> redistribution policy (IP), monitoring
> redundancy 1
>   tunnel server 1, 2
> regular expressions and routing policy 1
>   AS-path lists
>   community lists
>   community number format
>   metacharacters
>     defined
>     specifying as literals
> RIP (Routing Information Protocol)
>   clearing IP routing table
>   reinstalling routes in IP routing table
> route maps
>   and routing policy
>   deny keyword
>   filtering incoming/outgoing routes with access lists
>   instance
>   map tag
>   match clause
>   monitoring
>   permit keyword
>   sequence number
>   set clause
> route-map command
> routing policy
>   community
>   community list
>   configuring
>   managing the routing table
>   monitoring
>   overview
>   prefix lists
>   prefix trees
>   route maps
>   troubleshooting
> routing policy, BGP
>   access lists 1, 2
>   monitoring 1, 2
>   route maps
> routing table
>   managing the IP
> routing, IP 1, See also IP
>   monitoring 1, 2

S

> secure IP interfaces
> security parameters
> sequence number, route map
> Service Modules. See SMs
> set commands 1
>   and route maps
>   set as-path prepend
>   set automatic-tag
>   set comm-list delete
>   set community 1, 2
>   set dampening
>   set distance
>   set extcommunity 1, 2
>   set ip next-hop
>   set level
>   set local-preference
>   set metric
>   set metric-type
>   set origin
>   set route-class
>   set route-type
>   set tag
>   set weight
> shared tunnel-server ports 1, 2, 3, 4, 5, 6
> show access-list command
> show adjustment-factor command
> show bfd session command
> show dvmrp commands
>   show dvmrp destination profile
>   show dvmrp tunnel 1, 2, 3
>   show dvmrp tunnel summary 1, 2
> show gre commands
>   show gre destination profile
>   show gre tunnel 1, 2, 3
>   show gre tunnel summary 1, 2
> show ike commands
>   show ike policy-rule
>   show ike sa 1, 2
> show ip commands
>   show ip as-path-access-list
>   show ip cache flow
>   show ip cache flow aggregation
>   show ip community-list
>   show ip extcommunity-list
>   show ip prefix-list
>   show ip prefix-list detail
>   show ip prefix-list summary
>   show ip prefix-tree
>   show ip prefix-tree detail
>   show ip prefix-tree summary
>   show ip protocols
>   show ip redistribute
>   show ip route
>   show ip route slot
>   show ip static
>   show ip traffic
>   show ip tunnel reassembly statistics
> show ip flow sampling command 1, 2
> show ip match-policy-list command
> show ip mobile commands 1, 2, See also ip mobile commands
>   show ip mobile binding
>   show ip mobile home-agent
>   show ip mobile host
>   show ip mobile profile
>   show ip mobile secure foreign-agent
>   show ip mobile secure host
>   show ip mobile traffic
> show ip nat commands
>   show ip nat inside rule
>   show ip nat outside rule
>   show ip nat statistics
>   show ip nat translations 1, 2
> show ipsec commands
>   show ike certificates
>   show ike configuration
>   show ike identity
>   show ipsec ca identity
>   show ipsec certificates
>   show ipsec identity 1, 2
>   show ipsec ike-configuration
>   show ipsec ike-policy-rule
>   show ipsec ike-sa 1, 2
>   show ipsec key mypubkey rsa
>   show ipsec key pubkey-chain rsa
>   show ipsec lifetime
>   show ipsec local-endpoint
>   show ipsec option 1, 2
>   show ipsec transform-set
>   show ipsec tunnel detail
>   show ipsec tunnel summary
>   show ipsec tunnel virtual-router
>   show license ipsec-tunnels
> show ipsec transport commands
>   show ipsec transport interface
>   show ipsec transport interface summary
>   show ipsec transport profile
> show ipv6 commands
>   show license nat
> show l2c commands
>   show l2c
>   show l2c label
>   show l2c neighbor
>   show l2c statistics 1, 2
> show l2tp commands
>   show l2tp destination profile command
> show license commands
>   show license mobile-ip home-agent
> show route-map command
> single-shot tunnels
>   configuring
>   handling timeout periods
>   monitoring
>   overview
> single-shot-tunnel command
> SMs (Service modules)
>   installing 1, 2, 3, 4
>   monitoring parameters
>   redundancy 1, 2
> source, tunnel
> static routes 1, 2
> static tunnels
> statistics, tunnel reassembly
>   displaying
>   setting baseline for
> subscriber management
>   Mobile IP home agent
> support, technical See technical support

T

> table-map command
>   IP 1, 2
> technical support
>   contacting JTAC
> text and syntax conventions
> timeout periods for single-shot tunnels
> traffic, IP
> transform sets, IPSec
> transport network
> troubleshooting
>   DVMRP/IPSec, GRE/IPSec, and L2TP/IPSec tunnels
>   routing policy
> tunnel commands
>   tunnel mdt profile
> tunnel commands, IP
>   tunnel checksum 1, 2
>   tunnel destination 1, 2
>   tunnel mtu
>   tunnel sequence-datagrams
>   tunnel source 1, 2
> tunnel commands, IPSec
>   tunnel destination
>   tunnel destination backup
>   tunnel lifetime
>   tunnel local-identity
>   tunnel mtu
>   tunnel peer-identity
>   tunnel pfs group
>   tunnel session-key-inbound
>   tunnel session-key-outbound
>   tunnel signaling
>   tunnel source
>   tunnel transform set
> tunnel-server ports
>   shared 1, 2, 3
> tunnels, IP
>   DVMRP
>   DVMRP (IP in IP)
>   dynamic
>   endpoints
>   GRE
>   reassembling tunnel packets
>   shared tunnel-server ports 1, 2, 3, 4, 5, 6
>   static
> tunnels, IPSec monitoring
>   DVMRP/IPSec
>   GRE/IPSec
>   L2TP/IPSec
> tunnels, single-shot
>   configuring
>   handling timeout periods
>   monitoring
>   overview

U

> UDP (User Datagram Protocol)
>   encapsulation for NAT-T
>   statistics for NAT-T
> updates, BGP
>   AS-path filters

W

> well-known communities, BGP

X

> X.509v3 certificates