# Monitoring the Format of the Remote-Circuit-ID for RADIUS

#### Purpose

Display the format configured for the PPPoE remote circuit ID value captured from a DSLAM.

The default format is agent-circuit-ID. If the PPPoE remote circuit ID value is configured to include any or all of the agent-circuit-id, agent-remote-id, and nas-identifier components, the display lists the components included and the order in which they appear.

If the PPPoE remote circuit ID value is configured to use the format for the dsl-forum-1 keyword of radius remote-circuit-id-format, the display indicates that this format is in effect.

#### Action

To display the format configured for the PPPoE remote circuit ID value captured from a DSLAM:

    host1#show radius remote-circuit-id-format
    nas-identifier agent-circuit-id agent-remote-id

#### Related Documentation

- show radius remote-circuit-id-format