# request-type

#### Syntax

[ no | default ] request-type { access-request | acct-start | acct-stop }

#### Release Information

Command introduced in JunosE Release 12.1.0.

#### Description

Configures the RADIUS request message type. The no version restores the default value. By default, the access request type is configured.

#### Options

- access-request—Configures RADIUS to include the attribute in Access-Request packets
- acct-start—Configures RADIUS to include the attribute in Acct-Start packets
- acct-stop—Configures RADIUS to include the attribute in Acct-Stop packets

#### Mode

RADIUS Per-Profile List Configuration