Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- mpls policy-list

# Creating Policy Lists for MPLS

The following example creates an MPLS policy list.

1. Create the policy list routeForMpls.
   host1(config)#mpls policy-list routeForMpls host1(config-policy-list)#
2. Create the classification group.
   host1(config-policy-list)#classifier-group * precedence 200 host1(config-policy-list-classifier-group)#
3. Add one rule that sets the EXP bits for all packets to 2, and a second rule that uses the rate-limit profile mplsRLP
   host1(config-policy-list-classifier-group)#mark-exp 2 host1(config-policy-list-classifier-group)#rate-limit-profile mplsRLP5
4. Exit Policy List Configuration mode to save the configuration.
   host1(config-policy-list-classifier-group)#exit host1(config-policy-list)#exit host1(config)#
5. Display the policy list.

       host1#show policy-list routeForMpls

                                         Policy Table
                                         ------ -----
       MPLS Policy routeForMpls
          Administrative state: enable
          Reference count:      0
          Classifier control list: *, precedence 200
             mark-exp 2 mask 7
             rate-limit-profile mplsRLP5

| Note: In JunosE releases numbered lower than 11.3.x, when you attached a QoS profile to an interface configured for MPLS on an ES2 10G LM, the egress traffic from the MPLS interface that was classified as non-best-effort traffic was forwarded using the best-effort queue. In higher-numbered releases, when an output policy is specified with a non-best-effort traffic class and applied on an MPLS interface, the correct traffic class is used to classify and forward outgoing packets from the interface. For example, when an output policy is applied on an MPLS interface configured with a non-best-effort class, the outgoing traffic from the interface is correctly categorized according to the defined traffic class and does not use the best-effort queue.

## Related Documentation

- mpls policy-list

#### Published: 2011-09-30

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out