Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Configuring Local ATM Cross-Connects with AAL5 Encapsulation, Configuring Local Cross-Connects Between Ethernet/VLAN Interfaces, Configuring the Loopback Interface and Router ID for BGP for L2VPNs, Configuring the Loopback Interface and Router ID for VPLS, and Configuring MPLS LSPs for L2VPNs in the JunosE BGP and MPLS Configuration Guide

# ip address

#### Syntax

ip address ipAddress ipMask [ secondary ]

no ip address [ ipAddress ipMask [ secondary ] ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets a primary or secondary IP address for an interface or subinterface. The no version removes an IP address or disables IP processing. You must specify the layer 2 encapsulation before you can set the IP address.

#### Options

- ipAddress—IP address in 32-bit dotted decimal format (for example, 192.56.32.2)
- ipMask—mask for associated IP subnet in dotted decimal or prefix length notation
- secondary—Specifies that the configured address is a secondary IP address; if omitted, the configured address is the primary IP address

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

## Related Documentation

- Configuring Local ATM Cross-Connects with AAL5 Encapsulation, Configuring Local Cross-Connects Between Ethernet/VLAN Interfaces, Configuring the Loopback Interface and Router ID for BGP for L2VPNs, Configuring the Loopback Interface and Router ID for VPLS, and Configuring MPLS LSPs for L2VPNs in the JunosE BGP and MPLS Configuration Guide

#### Published: 2011-09-29

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out