Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Rate Limits for Interfaces Overview
- Monitoring Policy Management Overview

# Creating a One-Rate Rate-Limit Profile

To create or modify a one-rate rate-limit profile, use the following commands with the one-rate keyword:

- ip rate-limit-profile command
- ipv6 rate-limit-profile command
- l2tp rate-limit-profile command
- mpls rate-limit-profile command

The following example creates a rate-limit profile named tcpFriendly8Mb. This rate-limit profile, when included as part of a rule in a policy list, sets a TCP-friendly rate for a specified flow:

host1(config)#ip rate-limit-profile tcpFriendly8Mb one-rate host1(config-rate-limit-profile)#committed-rate 8000000 host1(config-rate-limit-profile)#committed-burst 1500000 host1(config-rate-limit-profile)#excess-burst 3000000 host1(config-rate-limit-profile)#committed-action transmit host1(config-rate-limit-profile)#conformed-action transmit host1(config-rate-limit-profile)#exceeded-action drop host1(config-rate-limit-profile)#mask-val 255

To configure a single-rate hard limit, set the committed rate and burst rate to the desired values, the committed action to transmit, the conformed action to drop, and the exceeded action to drop. The peak rate must be set to zero.

| Note: You can also achieve the characteristics of the single-rate hard limit by configuring a one-rate rate-limit profile with the extended burst rate set to zero.

## Related Documentation

- Rate Limits for Interfaces Overview
- Monitoring Policy Management Overview

#### Published: 2011-10-14

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out