# CLI Commands Used to Configure RADIUS IETF Attributes

Table 47 lists the RADIUS IETF attributes and the corresponding CLI commands used to configure them. The attributes are listed numerically—each attribute is followed by a list of the commands that you can use to manage the attribute.

Table 47: CLI Commands Used to Configure RADIUS IETF Attributes

Attribute Number | Attribute Name | CLI Command
--- | --- | ---
[4] | NAS-IP-Address | radius override nas-ip-addr tunnel-client-endpoint radius override nas-info
[5] | NAS-Port | radius include nas-port radius nas-port-format radius nas-port-format extended atm radius nas-port-format extended ethernet radius pppoe nas-port-format unique radius vlan nas-port-format stacked
[8] | Framed-IP-Address | radius include framed-ip-addr
[9] | Framed-Ip-Netmask | radius include framed-ip-netmask radius ignore framed-ip-netmask
[13] | Framed-Compression | radius include framed-compression
[22] | Framed-Route | radius include framed-route
[25] | Class | radius include class
[30] | Called-Station-Id | radius include called-station-id
[31] | Calling-Station-Id | radius calling-station-format radius calling-station-delimiter radius include calling-station-id radius override calling-station-id remote-circuit-id
[32] | NAS-Identifier | radius nas-identifier radius include nas-identifier radius override nas-info radius remote-circuit-id-format radius remote-circuit-id-delimiter
[41] | Acct-Delay-Time | radius include acct-delay-time
[44] | Acct-Session-Id | radius include acct-session-id radius acct-session-id-format
[45] | Acct-Authentic | radius include acct-authentic
[49] | Acct-Terminate-Cause | radius include acct-terminate-cause
[50] | Acct-Multi-Session-Id | radius include acct-multi-session-id
[51] | Acct-Link-Count | radius include acct-link-count
[52] | Acct-Input-Gigawords | radius include input-gigawords
[53] | Output-Gigawords | radius include output-gigawords
[55] | Event-Timestamp | radius include event-timestamp
[61] | NAS-Port-Type | radius dsl-port-type radius ethernet-port-type radius include nas-port-type
[64] | Tunnel-Type | radius include tunnel-type
[65] | Tunnel-Medium-Type | radius include tunnel-medium-type
[66] | Tunnel-Client-Endpoint | radius include tunnel-client-endpoint
[67] | Tunnel-Server-Endpoint | radius include tunnel-server-endpoint
[68] | Acct-Tunnel-Connection | radius include acct-tunnel-connection
[77] | Connect-Info | radius connect-info-format l2tp-connect-speed radius include connect-info
[82] | Tunnel-Assignment-Id | radius include tunnel-assignment-id
[83] | Tunnel-Preference | radius include tunnel-preference
[87] | NAS-Port-Id | aaa intf-desc-format include radius include nas-port-id radius override nas-port-id remote-circuit-id
[90] | Tunnel-Client-Auth-Id | radius include tunnel-client-auth-id
[91] | Tunnel-Server-Auth-Id | radius include tunnel-server-auth-id
[96] | Framed-Interface-Id | radius include framed-interface-id
[97] | Framed-Ipv6-Prefix | radius include framed-ipv6-prefix
[99] | Framed-Ipv6-Route | radius include framed-ipv6-route
[100] | Framed-Ipv6-Pool | radius include framed-ipv6-pool
[123] | Delegated-Ipv6-Prefix | radius include delegated-ipv6-prefix
[188] | Ascend-Num-In-Multilink | radius include ascend-num-in-multilink
| All Tunnel Server Attributes | radius include tunnel-server-attributes

#### Related Documentation

- Propagation of LAG Subscriber Information to AAA and RADIUS
- RADIUS IETF Attributes Supported for Subscriber AAA Access Messages
- RADIUS IETF Attributes Supported for Subscriber AAA Accounting Messages
- RADIUS IETF Attributes Supported for AAA Tunnel Accounting Messages
- RADIUS Attributes Supported for CLI AAA Messages
- RADIUS IETF Attributes
- Monitoring Override Settings of RADIUS IETF Attributes
- Monitoring the NAS-Port-Format RADIUS Attribute
- Monitoring the Calling-Station-Id RADIUS Attribute
- Monitoring the NAS-Identifier RADIUS Attribute
- Monitoring the Format of the Remote-Circuit-ID for RADIUS
- Monitoring the Delimiter Character in the Remote-Circuit-ID for RADIUS
- Monitoring the DSL-Port-Type RADIUS Attribute
- Monitoring the Connect-Info RADIUS Attribute
- Monitoring the NAS-Port-ID RADIUS Attribute
- aaa intf-desc-format include
- radius acct-session-id-format
- radius calling-station-delimiter
- radius calling-station-format
- radius connect-info-format
- radius dsl-port-type
- radius ethernet-port-type
- radius ignore
- radius include
- radius nas-identifier
- radius nas-port-format
- radius nas-port-format extended
- radius override calling-station-id remote-circuit-id
- radius override nas-info
- radius override nas-ip-addr tunnel-client-endpoint
- radius override nas-port-id remote-circuit-id
- radius pppoe nas-port-format unique
- radius remote-circuit-id-delimiter
- radius remote-circuit-id-format
- radius vlan nas-port-format stacked