# remote host

#### Syntax

[ no ] remote host { hostname | default }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines an L2TP host profile. Accesses the L2TP Destination Profile Host Configuration mode. The no version removes an L2TP host profile.

#### Options

- hostname—Name the LAC must supply in the hostname AVP of the receive SCCRQ; can be up to 64 characters in length (no spaces)
- default—Allows the LAC to use any hostname in the hostname AVP

#### Mode

L2TP Destination Profile Configuration