# PPP Terminate Reasons

Table 61 lists the default PPP terminate mappings. The table indicates the supported PPP terminate reasons and the RADIUS Acct-Terminate-Cause attributes they are mapped to by default.

Table 61: Default PPP Mappings

PPP Terminate Reason | RADIUS Acct-Terminate-Cause
--- | ---
| Code | Description
authenticate authenticator timeout | 17 | user error
authenticate challenge timeout | 10 | nas request
authenticate chap no resources | 10 | nas request
authenticate chap peer authenticator timeout | 17 | user error
authenticate deny by peer | 17 | user error
authenticate inactivity timeout | 4 | idle timeout
authenticate max requests | 10 | nas request
authenticate no authenticator | 10 | nas request
authenticate pap peer authenticator timeout | 17 | user error
authenticate pap request timeout | 10 | nas request
authenticate session timeout | 5 | session timeout
authenticate too many requests | 10 | nas request
authenticate tunnel fail immediate | 10 | nas request
authenticate tunnel unsupported tunnel type | 10 | nas request
bundle fail create | 10 | nas request
bundle fail engine add | 10 | nas request
bundle fail fragment size mismatch | 10 | nas request
bundle fail fragmentation location | 10 | nas request
bundle fail fragmentation mismatch | 10 | nas request
bundle fail join | 10 | nas request
bundle fail link selection mismatch | 10 | nas request
bundle fail local mped not set yet | 10 | nas request
bundle fail local mrru mismatch | 10 | nas request
bundle fail local mru mismatch | 10 | nas request
bundle fail peer mrru mismatch | 10 | nas request
bundle fail reassembly location | 10 | nas request
bundle fail reassembly mismatch | 10 | nas request
bundle fail record network | 10 | nas request
bundle fail server location mismatch | 10 | nas request
bundle fail static link | 10 | nas request
failover during authentication | 6 | admin reset
interface admin disable | 6 | admin reset
interface down | 2 | lost carrier
interface no hardware | 8 | port error
ip admin disable | 10 | nas request
ip inhibited by authentication | 10 | nas request
ip link down | 10 | nas request
ip max configure exceeded | 10 | nas request
ip no local ip address | 10 | nas request
ip no local ip address mask | 10 | nas request
ip no local primary dns address | 10 | nas request
ip no local primary nbns address | 10 | nas request
ip no local secondary dns address | 10 | nas request
ip no local secondary nbns address | 10 | nas request
ip no peer ip address | 10 | nas request
ip no peer ip address mask | 10 | nas request
ip no peer primary dns address | 10 | nas request
ip no peer primary nbns address | 10 | nas request
ip no peer secondary dns address | 10 | nas request
ip no peer secondary nbns address | 10 | nas request
ip no service | 10 | nas request
ip peer renegotiate rx conf ack | 10 | nas request
ip peer renegotiate rx conf nak | 10 | nas request
ip peer renegotiate rx conf rej | 10 | nas request
ip peer renegotiate rx conf req | 10 | nas request
ip peer terminate term ack | 10 | nas request
ip peer terminate code rej | 10 | nas request
ip peer terminate term req | 10 | nas request
ip service disable | 10 | nas request
ip stale stacking | 10 | nas request
ipv6 admin disable | 10 | nas request
ipv6 inhibited by authentication | 10 | nas request
ipv6 link down | 10 | nas request
ipv6 local and peer interface ids identical | 10 | nas request
ipv6 max configure exceeded | 10 | nas request
ipv6 no local ipv6 interface id | 10 | nas request
ipv6 no peer ipv6 interface id | 10 | nas request
ipv6 no service | 10 | nas request
ipv6 peer renegotiate rx conf ack | 10 | nas request
ipv6 peer renegotiate rx conf nak | 10 | nas request
ipv6 peer renegotiate rx conf rej | 10 | nas request
ipv6 peer renegotiate rx conf req | 10 | nas request
ipv6 peer terminate code rej | 10 | nas request
ipv6 peer terminate term ack | 10 | nas request
ipv6 peer terminate term req | 10 | nas request
ipv6 service disable | 10 | nas request
ipv6 stale stacking | 10 | nas request
lcp authenticate terminate hold | 10 | nas request
lcp configured mrru too small | 10 | nas request
lcp configured mru invalid | 10 | nas request
lcp configured mru too small | 10 | nas request
lcp dynamic interface hold | 10 | nas request
lcp keepalive failure | 10 | nas request
lcp loopback rx conf req | 10 | nas request
lcp loopback rx echo reply | 10 | nas request
lcp loopback rx echo req | 10 | nas request
lcp max configure exceeded | 10 | nas request
lcp mru changed | 10 | nas request
lcp negotiation timeout | 10 | nas request
lcp no localaccm | 10 | nas request
lcp no localacfc | 10 | nas request
lcp no local authentication | 10 | nas request
lcp no local endpoint discriminator | 10 | nas request
lcp no local magic number | 10 | nas request
lcp no local mrru | 10 | nas request
lcp no local mru | 10 | nas request
lcp no localpfc | 10 | nas request
lcp no peer accm | 10 | nas request
lcp no peer authentication | 10 | nas request
lcp no peer endpoint discriminator | 10 | nas request
lcp no peer magicnumber | 10 | nas request
lcp no peer mrru | 10 | nas request
lcp no peer mru | 10 | nas request
lcp no peer pfc | 10 | nas request
lcp peer terminate code rej | 1 | user request
lcp peer terminate term ack | 1 | user request
lcp peer terminate term req | 1 | user request
lcp peer terminate protocol reject | 1 | user request
lcp peer renegotiate rx conf ack | 1 | user request
lcp peer renegotiate rx conf nak | 1 | user request
lcp peer renegotiate rx conf rej | 1 | user request
lcp peer renegotiate rx conf req | 1 | user request
lcp tunnel disconnected | 10 | nas request
lcp tunnel failed | 10 | nas request
link interface no hardware | 8 | port error
lower interface attach failed | 2 | lost carrier
lower interface teardown | 2 | lost carrier
mpls admin disable | 10 | nas request
mpls link down | 10 | nas request
mpls max configure exceeded | 10 | nas request
mpls no service | 10 | nas request
mpls peer renegotiate rx conf ack | 10 | nas request
mpls peer renegotiate rx conf nak | 10 | nas request
mpls peer renegotiate rx conf rej | 10 | nas request
mpls peer renegotiate rx conf req | 10 | nas request
mpls peer terminate code rej | 10 | nas request
mpls peer terminate term ack | 10 | nas request
mpls peer terminate term req | 10 | nas request
mpls service disable | 10 | nas request
mpls stale stacking | 10 | nas request
network interface admin disable | 6 | admin reset
no bundle | 10 | nas request
no interface | 8 | port error
no link interface | 8 | port error
no ncps available | 10 | nas request
no network interface | 10 | nas request
no upper interface | 9 | nas error
osi admin disable | 10 | nas request
osi link down | 10 | nas request
osi max configure exceeded | 10 | nas request
osi no local align npdu | 10 | nas request
osi no peer align npdu | 10 | nas request
osi no service | 10 | nas request
osi peer renegotiate rx conf ack | 10 | nas request
osi peer renegotiate rx conf nak | 10 | nas request
osi peer renegotiate rx conf rej | 10 | nas request
osi peer renegotiate rx conf req | 10 | nas request
osi peer terminate code rej | 10 | nas request
osi peer terminate term ack | 10 | nas request
osi peer terminate term req | 10 | nas request
osi service disable | 10 | nas request
osi stale stacking | 10 | nas request