# CLI Commands Used to Include or Exclude Attributes in RADIUS Messages

You can use the radius include command to enable or disable the inclusion of RADIUS attributes in Acct-on, Acct-off, Access-Request, Acct-Start, and Acct-Stop messages.

Table 50 lists the RADIUS attributes that can be included or excluded in RADIUS messages using the radius include command and the RADIUS messages in which the attributes are supported.

Table 50: RADIUS Attributes Included in Corresponding RADIUS Messages

Attribute Number | Attribute Name | Access-Request | Acct-on | Acct-off | Acct-Start | Acct-Stop
--- | --- | --- | --- | --- | --- | ---
[5] | NAS-Port | ✓ | – | – | ✓ | ✓
[8] | Framed-IP-Address | ✓ | – | – | ✓ | ✓
[9] | Framed-IP-Netmask | – | – | – | ✓ | ✓
[13] | Framed-Compression | – | – | – | ✓ | ✓
[22] | Framed-Route | – | – | – | ✓ | ✓
[25] | Class | – | – | – | ✓ | ✓
[26-10] | Ingress-Policy-Name | – | – | – | ✓ | ✓
[26-11] | Egress-Policy-Name | – | – | – | ✓ | ✓
[26-24] | Pppoe-Description | ✓ | – | – | ✓ | ✓
[26-35] | Acct-Input-Gigapackets | – | – | – | – | ✓
[26-43] | Acct-Output-Gigapackets | – | – | – | – | ✓
[26-44] | Tunnel-Interface-ID | ✓ | – | – | ✓ | ✓
[26-45] | Ipv6-Virtual-Router | – | – | – | – | ✓
[26-46] | Ipv6-Local-Interface | – | – | – | – | ✓
[26-47] | Ipv6-Primary-DNS | – | – | – | – | ✓
[26-48] | Ipv6-Secondary-DNS | – | – | – | – | ✓
[26-51] | Disconnect-Cause | – | – | – | – | ✓
[26-53] | Service-Description | ✓ | – | – | ✓ | ✓
[26-55] | DHCP-Options | ✓ | – | – | ✓ | ✓
[26-56] | DHCP-MAC-Address | ✓ | – | – | ✓ | ✓
[26-57] | DHCP-GI-Address | ✓ | – | – | ✓ | ✓
[26-62] | MLPPP-Bundle-Name | ✓ | – | – | ✓ | ✓
[26-63] | Interface-Description | ✓ | – | – | ✓ | ✓
[26-81] | L2c-Information | ✓ | – | – | – | –
[26-92] | L2C-Up-Stream-Data | ✓ | – | – | ✓ | ✓
[26-93] | L2C-Down-Stream-Data | ✓ | – | – | ✓ | ✓
[26-110] | Acc-Loop-Cir-Id | ✓ | – | – | ✓ | ✓
[26-111] | Acc-Aggr-Cir-Id-Bin | ✓ | – | – | ✓ | ✓
[26-112] | Acc-Aggr-Cir-Id-Asc | ✓ | – | – | ✓ | ✓
[26-113] | Act-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-114] | Act-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-115] | Min-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-116] | Min-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-117] | Att-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-118] | Att-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-119] | Max-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-120] | Max-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-121] | Min-LP-Data-Rate-Up | ✓ | – | – | ✓ | ✓
[26-122] | Min-LP-Data-Rate-Dn | ✓ | – | – | ✓ | ✓
[26-123] | Max-Interlv-Delay-Up | ✓ | – | – | ✓ | ✓
[26-124] | Act-Interlv-Delay-Up | ✓ | – | – | ✓ | ✓
[26-125] | Max-Interlv-Delay-Dn | ✓ | – | – | ✓ | ✓
[26-126] | Act-Interlv-Delay-Dn | ✓ | – | – | ✓ | ✓
[26-127] | DSL-Line-State | ✓ | – | – | ✓ | ✓
[26-128] | DSL-Type | ✓ | – | – | ✓ | ✓
[26-129] | Ipv6-NdRa-Prefix | – | – | – | – | ✓
[26-141] | Downstream-Calculated-Qos | ✓ | – | – | ✓ | ✓
[26-142] | Upstream-Calculated-Qos-Rate | ✓ | – | – | ✓ | ✓
[26-150] | ICR-Partition-Id | ✓ | – | – | ✓ | ✓
[26-159] | DHCP-Option 82 | ✓ | – | – | ✓ | ✓
[30] | Called-Station-Id | ✓ | – | – | ✓ | ✓
[31] | Calling-Station-Id | ✓ | – | – | ✓ | ✓
[32] | NAS-Identifier | ✓ | ✓ | ✓ | ✓ | ✓
[41] | Acct-Delay-Time | – | ✓ | ✓ | – | –
[44] | Acct-Session-Id | ✓ | ✓ | ✓ | – | –
[45] | Acct-Authentic | – | ✓ | ✓ | – | –
[49] | Acct-Terminate-Cause | – | – | ✓ | – | –
[50] | Acct-Multi-Session-Id | ✓ | – | – | ✓ | ✓
[51] | Acct-Link-Count | – | – | – | ✓ | ✓
[52] | Acct-Input-Gigawords | – | – | – | – | ✓
[53] | Acct-Output-Gigawords | – | – | – | – | ✓
[55] | Event-Timestamp | – | ✓ | ✓ | ✓ | ✓
[61] | NAS-Port-Type | ✓ | – | – | ✓ | ✓
[64] | Tunnel-Type | ✓ | – | – | ✓ | ✓
[65] | Tunnel-Medium-Type | ✓ | – | – | ✓ | ✓
[66] | Tunnel-Client-Endpoint | ✓ | – | – | ✓ | ✓
[67] | Tunnel-Server-Endpoint | ✓ | – | – | ✓ | ✓
[68] | Acct-Tunnel-Connection | ✓ | – | – | ✓ | ✓
[77] | Connect-Info | ✓ | – | – | ✓ | ✓
[82] | Tunnel-Assignment-Id | – | – | – | ✓ | ✓
[83] | Tunnel-Preference | – | – | – | ✓ | ✓
[87] | NAS-Port-Id | ✓ | – | – | ✓ | ✓
[90] | Tunnel-Client-Auth-Id | ✓ | – | – | ✓ | ✓
[91] | Tunnel-Server-Auth-Id | ✓ | – | – | ✓ | ✓
[96] | Framed-Interface-Id | ✓ | – | – | ✓ | ✓
[97] | Framed-Ipv6-Prefix | ✓ | – | – | ✓ | ✓
[99] | Framed-Ipv6-Route | – | – | – | – | ✓
[100] | Framed-IPv6-Pool | – | – | – | – | ✓
[123] | Delegated-IPv6-Prefix | – | – | – | – | ✓
[188] | Ascend-Num-In-Multilink | ✓ | – | – | ✓ | ✓
| All Tunnel-Server-Attributes | ✓ | – | – | ✓ | ✓
| All Ipv6-Accounting Attributes | – | – | – | – | ✓

#### Related Documentation

- Subscriber AAA Access Messages Overview
- Subscriber AAA Accounting Messages Overview
- RADIUS IETF Attributes
- Juniper Networks VSAs
- Monitoring Included RADIUS Attributes
- radius include