Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# ip vrrp timers-learn

#### Syntax

[ no ] ip vrrp vrid timers-learn

#### Release Information

Command introduced in JunosE Release 10.3.0.

#### Description

Configures the VRRP instance to learn the VRRP advertisement interval from the master VRRP instance. This feature is useful only when you have configured different advertisement intervals for the master VRRP instance and the backup VRRP instance. This feature enables the unified ISSU operation to proceed successfully. The no version disables the learning timer for the VRRP instance. If you have configured different advertisement intervals for the VRRP master and VRRP backup instances, the VRRP session breaks, and both instances behave like the master instance, and the router displays an error message.

#### Options

- vrid—VRID identifier; a number in the range 1–255

#### Mode

Interface Configuration, Subinterface Configuration

#### Published: 2011-10-18

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out