# Monitoring MLD Proxy Groups

#### Purpose

Display information about all or specified multicast groups that MLD proxy reported.

#### Action

To display information about all multicast groups that MLD proxy reported:

    host1#show ipv6 mld-proxy groups

    Grp Address     Interface       Grp Mode
    --------------- --------------- --------------
    ff0e::1         ATM5/1.200
    ff0e::2         ATM5/1.200
    ff0e::3         ATM5/1.200      Include(1):
      2001::1
    ff0e::4         ATM5/1.200
    ff0e::5         ATM5/1.200      Exclude(1):
      2001::2

    Counts: 3 <*,G>, 1 Exclude (1 sources), 1 Include (1 sources)
           (5 total)

To display information about specified multicast groups that MLD proxy reported:

    host1#show ipv6 mld-proxy groups ff0e::1
    Grp Address     Interface       Grp Mode
    --------------- --------------- --------------
    ff0e::1         ATM5/1.200

    Counts: 1 <*,G>
           (1 total)

To display the number of multicast groups that MLD proxy reported:

    host1#show ipv6 mld-proxy groups count
    Counts: 3 <*,G>, 1 Exclude (1 sources), 1 Include (1 sources)
           (5 total)

#### Meaning

Table 36 lists the show ipv6 mld-proxy groups command output fields.

Table 36: show ipv6 mld-proxy groups Output Fields

Field Name | Field Description
--- | ---
Grp Address | Address of the multicast group
Interface | Type and identifier of the upstream interface associated with the multicast group
Grp Mode | Blank—No sources included or excluded for this group Include—Sources included for this group Exclude—Sources excluded for this group
Count | Total number of multicast groups associated with this interface

#### Related Documentation

- show ipv6 mld-proxy groups