Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# ip vrrp advertise-interval

#### Syntax

ip vrrp vrid advertise-interval advertiseInterval [ seconds | milliseconds ]

no ip vrrp vrid advertise-interval

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the VRRP advertisement interval time. You must use seconds to comply with RFC 2338. Use milliseconds only if all VRRP instances peering for the given VRID are composed of E Series routers. The no version restores the default value, 1 second.

#### Options

- vrid—VRID identifier; a number in the range 1–255
- advertiseInterval—Advertisement period in seconds or milliseconds; in the range 1–255 seconds or 100–255000 milliseconds
- seconds—Specifies interval in seconds
- milliseconds—Specifies interval in milliseconds

#### Mode

Interface Configuration

#### Published: 2011-09-29

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out