Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# ipv6 mld-proxy unsolicited-report-interval

#### Syntax

ipv6 mld-proxy unsolicited-report-interval tenths-of-a-second

no ipv6 mld-proxy unsolicited-report-interval

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies how often the upstream interface should transmit unsolicited reports. This command has no effect on interfaces other than the upstream value. The no version transmits unsolicited reports using the default value, 100-tenths of a second (10 seconds).

| Note: Issue this command only on the upstream interface. Otherwise, this command will have no effect.

#### Options

- tenths-of-a-seconds—Time interval at which the interface transmits unsolicited reports

#### Mode

Interface Configuration

#### Published: 2011-09-29

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out