Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# threshold-test

#### Syntax

threshold-test startup { falling | rising | risingorfalling }

threshold-test absolute-value rising risingValue falling fallingValue

threshold-test event { rising eventOwner eventName | falling eventOwner eventName | delta-rising eventOwner eventName | delta-falling eventOwner eventName }

threshold-test delta-value rising risingValue falling fallingValue

no threshold-test [ startup | absolute-value | delta-value | event rising | event falling | event delta-rising | event delta-falling ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines the values for an SNMP threshold-test trigger. The no version deletes the threshold-test values for this trigger or removes either the threshold startup condition or event binding.

#### Options

- startup—Startup threshold condition that you predict the sample to follow
  - falling—Specifies that the sample values are expected to be falling values
  - rising—Specifies that the sample values are expected to be rising values
  - risingorfalling—Specifies that the sample values might be either rising values or falling values
- absolute-value—Specifies that the trigger is monitoring absolute threshold values
- risingValue—Rising threshold value for the trigger, in the range -2147483648–2147483648
- fallingValue—Falling threshold value for the trigger, in the range -2147483648–2147483648
- event—Binds an event owner and name to specific events on which the threshold-test might trigger: rising values within a sample, falling values within a sample, rising values between samples, or falling values between samples
- eventOwner—Event owner name; string of up to 32 alphanumeric characters
- eventName—Event name; string of up to 32 alphanumeric characters
- delta-value—Specifies that the trigger is monitoring the difference (delta)( between sample values

#### Mode

SNMP Trigger Configuration

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out