Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# timing source

#### Syntax

timing source selector { internal | line lineType | uidType interfaceSpecifier }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures the router’s timing sources. Only one of these timing sources can be an external source received through an interface on an I/O module other than the SRP I/O module; the other two must be either internal sources or external sources received through the SRP I/O modules. There is no no version.

#### Options

- selector—Priority of the timing source; in descending order: primary, secondary, or tertiary
- internal—Specifies the internal SC oscillator
- line—Specifies external timing input on the SRP module
- lineType—One of the following timing sources:
  - e1:a—E1 clock, port A on SRP module
  - e1:b—E1 clock, port B on SRP module
  - t1:a—T1 clock, port A on SRP module
  - t1:b—T1 clock, port B on SRP module
- uidType—One of the following interfaces:
  - ds1—Specifies a DS1 interface
  - ds3—Specifies a DS3 interface
  - e1—Specifies an E1 interface
  - e3—Specifies an E3 interface
  - sonet—Specifies a SONET interface
- interfaceSpecifier—Particular interface; in the form slot/port[:subPort ]

#### Mode

Global Configuration

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out