Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# ipv6 nd dad attempts

#### Syntax

ipv6 nd dad attempts numberOfAttempts

no ipv6 nd dad attempts

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the number of consecutive neighbor solicitation messages that an interface sends while the router performs duplicate address detection (DAD) on the unicast IPv6 addresses of the interface. The no version returns the number of neighbor solicitation messages to its default value (one message without any follow-up messages).

#### Options

- numberOfAttempts—Number of neighbor solicitation messages that you want the router to transmit

#### Mode

Interface Configuration

#### Published: 2011-09-29

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out