Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# ppp reassembly

#### Syntax

ppp reassembly [ mrru ]

no ppp reassembly

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables reassembly on an MLPPP link interface and optionally specifies the administrative MRRU value, in octets, for the link. The no version disables reassembly on the link and restores the default value, which is the link’s local MRU.

#### Options

- mrru—Maximum allowable size of the PPP packet payload that the router can receive, in the range 64–65535; default value is the link’s local MRU

#### Mode

Interface Configuration, Profile Configuration, Subinterface Configuration

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out