Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# sscc option

#### Syntax

sscc option { user-ip-mask-override | send-calling-station-id | send-local-qos-profile-config | send-lac-nas-ip | send-lac-nas-port }

no sscc option

#### Release Information

Command introduced in JunosE Release 10.2.0.

send-calling-station-id keyword added in JunosE Release 11.1.0.

send-local-qos-profile-config keyword added in JunosE Release 11.2.0.

send-lac-nas-ip and send-lac-nas-port keyword added in JunosE Release 12.2.0.

#### Description

When used with the user-ip-mask-override option, enables the user IP address mask to be sent to the Policy Decision Point (PDP) in place of the interface IP address mask for a virtual router. If user IP address mask is not available, then the interface IP address mask is sent. The no version disables user IP address mask override.

When used with the send-calling-station-id option, enables the calling station ID to be sent to the PDP for a virtual router. The no version disables the option to send the calling station ID.

When used with the send-local-qos-profile-config option, enables the local QoS profile attachment information to be sent to the PDP for a virtual router. The no version disables the option to send the local QoS profile attachment information.

When used with the send-lac-nas-ip option, enables the LAC side NAS-IP address information to be sent to the PDP for a virtual router. The no version disables the option to send the NAS-IP address information.

When used with the send-lac-nas-port option, enables the LAC side NAS-Port information to be sent to the PDP for a virtual router. The no version disables the option to send the LAC side NAS-Port information.

#### Options

- user-ip-mask-override—Enables user IP address mask to be sent to PDP
- send-calling-station-id—Enables calling station ID to be sent to PDP
- send-local-qos-profile-config—Enables local QoS profile attachment information to be sent to the PDP
- send-lac-nas-ip—Enables the LAC side NAS-IP address information to be sent to the PDP
- send-lac-nas-port—Enables the LAC side NAS-Port information to be sent to the PDP

#### Mode

Global Configuration

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out