# dhcpv6LsGeneral

#### Description

DHCPv6 local server events

#### Emergency

None

#### Alert

None

#### Critical

None

#### Error

Failure to create server (bad router or out of memory); errors encountered while processing ISSU signals or while mirroring; initialization error during the configuration of the DUID type

#### Warning Log

Attempt to remove a nonexistent server; any failure during the configuration of the DUID type

#### Notice Log

Failure to create server (IPv6 not licensed); cold/warm restart of DHCPv6 local server; before/after restoring client bindings; warm SRP switchover problems during the configuration of the DUID type

#### Info

None

#### Debug

Server bind, creation, deletion, unbind, and restoration of bindings post warm SRP switchover; Prefix Allocation Notification: designated prefix is already in use by another client; if ISSU is running on a DHCPv6 local server, ISSU and HA debug messages are logged; authentication of subscribers with the AAA username

#### Filter

None