Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- Rate Shaping and Port Shaping Overview
- Configuring a Scheduler Profile for a Scheduler Node or Queue
- scheduler-profile
- shaping-rate

# Configuring Rate Shaping for a Scheduler Node or Queue

The router supports 64,000 rate shapers per line module. Shaping rates are multiples of 1 Kbps.

To configure a shaping rate for a scheduler node or queue:

1. Create a scheduler profile.
   host1(config)#scheduler-profile video host1(config-scheduler-profile)#
2. Specify a shaping rate in the scheduler profile.
   host1(config-scheduler-profile)#shaping-rate 128000 burst 32767 milliseconds host1(config-scheduler-profile)#shaping-rate 5000 x 90

   The range for the shared-shaping rate is 1000–1000000000 bps (1 Kbps–1000 Kbps); the default is the minimum shaping rate (1 Kbps). The router rounds the rate to the next higher 8 Kbps.

   Use the operator and operandValue variables to configure a shaping rate with an expression.

   You can use the bps or kbps keywords to specify the unit of the shaping rate. By default, the shaping rate is configured in bps.

   Use the burst keyword to specify the catch-up number associated with the shaper; the range is 0–522240. Specifying 0 enables the router to select an applicable default value.

   Use the milliseconds or bytes keywords to specify the unit of the burst size.

## Related Documentation

- Rate Shaping and Port Shaping Overview
- Configuring a Scheduler Profile for a Scheduler Node or Queue
- scheduler-profile
- shaping-rate

#### Published: 2011-09-20

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out