# Index

Symbols A B C D E F G H I J L M N O P Q R S T U V W

Symbols

> 10/100Base-T port 1, 2
> –48 VDC power 1, 2, 3, 4

A

> abnormal LED activity 1, 2
> access, management 1, 2
>   setting up console 1, 2
>   SNMP 1, 2
>   Telnet setup
> accessing, fan tray
> adapters, I/O 1, 2
> agency certification 1, 2, 3, 4
> air filter 1
>   maintaining
>   replacing
> airflow 1
>   rack-mounted installation and
>   specifications 1, 2
> alarm ports
> amperage 1, 2
> antistatic bags and containers
> assembly numbers, locating
> assigning an IP address
> auxiliary port 1, 2

B

> bays, upper and lower, right and left 1, 2, 3
> BNC connector
> booting
>   LED activity

C

> cable management bracket
> cables
>   connecting
>   failure
>   IOA module
>   pinouts
>   power distribution unit
>   recommendations
>   required
>   SRP IOA 1, 2
> cabling
>   SRP IOA
> cabling router
> cabling SRP IOA
> Case Manager
> certification 1, 2, 3, 4
> chassis
> circulation, air
> classification, packet
> cleaning the router
> CLI (command-line interface)
> clock source input ports
> clocking problems
> command-line interface
> compliance
>   product reclamation and recycling
>   regulatory
> components
>   returning 1, 2
>   storing
> configuring cables 1, 2
> configuring management access
> configuring Telnet
> connecting console to the router
> connectors, pinouts
> console
>   for management access 1, 2
>   ports
>     10/100Base-T
>     RS-232
> console port 1, 2
> consumption, power 1, 2
> conventions
>   notice icons
>   text and syntax
> cooling system
>   air filter, maintaining
> crossover cable
> current (electrical) requirements 1, 2
> customer support 1, 2
>   contacting JTAC

D

> damaged components, returning
> DB-9 connector 1, 2
> DC power 1, 2, 3
> detecting double-bit error
> diagnosing problems
> diagnostic LEDs
> dimensions of E120 router
> dimensions of E320 router
> dissipation, heat 1, 2
> distribution rack 1, 2
> documentation set
>   comments on
> double-bit errors
>   detecting
>   troubleshooting

E

> E120 router
>   assigning IP address to
>   cabling
>   cabling recommendations
>   cleaning
>   dimensions
>   electrical requirements
>   environmental requirements
>   equipment rack requirements
>   Ethernet cable
>   installing
>   installing modules
>   lifting
>   management access
>   mechanical requirements
>   modules
>   power requirements
>   powering down
>   powering up
>   safety guidelines
>   site planning
>   slot numbering
>   space requirements 1, 2
>   troubleshooting 1, 2
>   unpacking
>   views
> E320 router
>   assigning IP address to
>   cabling
>   cabling recommendations
>   cleaning
>   dimensions
>   electrical requirements
>   environmental requirements
>   equipment rack requirements
>   Ethernet cable
>   installing
>   installing modules
>   lifting
>   management access
>   mechanical requirements
>   modules
>   power requirements
>   powering down
>   powering up
>   safety guidelines
>   site planning
>   slot numbering
>   space requirements 1, 2
>   troubleshooting 1, 2
>   unpacking
>   views
> EIA distribution rack
> ejectors, module
> electrical requirements 1, 2
> electronic equipment, recycling
> electrostatic discharge, precautions
> environmental requirements
> ESD grounding jack
> Ethernet link
> external timing ports

F

> fabric slices
> failover, SRP modules
> failures
>   fans
>   general
> FAN FAIL LED
> FAN OK LED
> fan tray 1
>   hot-swapping
> fans
>   failure 1, 2
>   installing
>   location
>   redundancy
>   removing
>   status
> far end receive failure
> FERF (far end receive failure)
> filter, air
> flash cards 1
>   redundancy

G

> Global Configuration mode
> ground wires required
> grounding jacks

H

> halt command 1, 2
> hardware
>   cable configuration 1, 2
>   reclamation and recycling
>   redundancy features
>   repairing and replacing
> hazardous materials, reclamation and recycling
> heat dissipation 1, 2, 3
> high-availability mode
> hot-swapping fan trays
> hot-swapping modules
> humidity requirements 1, 2
> HyperTerminal

I

> I/O adapter 1, 2
> installing IOA shelf
> installing modules
>   IOAs
>   line modules
>   order of installation
>   SFM modules
>   slot numbering
>   SRP IOA
>   SRP modules
> installing NVS cards 1
> installing router 1
>   site planning
> installing SFPs
> IOA module 1, 2
>   cables
>   combinations of
>   installing
>   removing
>   SFPs
>   SRP
> IOA shelf 1
>   installing
> IP address, assigning

J

> JTAC, contacting

L

> lead in equipment, reclamation and recycling
> LEDs 1
>   abnormal activity 1, 2
>   fans
>   normal activity
> lifting router
> Line Configuration mode
> line modules 1, 2
>   installing
>   LEDs
>   pairing with other modules
>   removing
>   slot numbering
> LM (line module)
> location, for routers

M

> maintenance, system
> management
>   ports
>     10/100Base-T
>     auxiliary
>     RS-232
> management access 1, 2
>   setting up console 1, 2
>   SNMP 1, 2
>   Telnet setup
> Management Information Bases
> management port
> managing modules
> manuals
>   comments on
> mechanical requirements for distribution rack
> MIBs (Management Information Bases)
> module reset button
> modules 1
>   failure
>   hot-swapping
>   installing 1, 2
>     order of installation
>   IOAs
>   line
>   managing
>   removing
>   repairing and replacing
>   replacing
>   resetting
>   self-testing
>   SFM
>   SRP
>   storing
> monitoring LEDs
> monitoring temperature
> mounting kits
> mounting posts for rack

N

> network management 1, 2
>   setting up console 1, 2
>   SNMP 1, 2
>   Telnet setup
> network timing ports
> NMI button
> nonvolatile storage
> notice icons
> NVS cards 1
>   installing 1, 2
>   redundancy
>   storing

O

> order of module installation

P

> packaging, recycling
> packet classification
> packing instructions
> passwords, Telnet
> PC-CARD
> PCMCIA slot, SRP modules
> PDU 1
>   cabling
>   replacing
> pinouts, E Series router cables and connectors
> planning site for installation
> plenum
> ports
>   alarm
>   console
>   external timing
>   status LEDs
> power
>   cabling power distribution unit 1, 2
>   consumption, system 1, 2
>   dissipation 1, 2
>   failures 1, 2
>   problems
>   source A
>   source B
>   specifications 1, 2
> power distribution unit
>   replacing
> Power Distribution Unit (PDU)
> power input module, cabling
> power switches 1, 2
> powering down router
> powering up router
> preinstallation responsibilities
> preparing site for installation
> Privileged Exec command mode
> problems
> product numbers, locating

Q

> QoS, packet classification for

R

> rack, distribution
> reclamation and recycling
> recycling Juniper Networks equipment
> redundancy 1
>   fans
>   NVS cards
>   power
>   SRP module
> regulatory requirements
> release mechanisms for SFPs
> removing components
> removing modules
> removing SFPs
> repacking components
> repairing hardware components
> replacing components
> replacing modules
> replacing NVS cards 1, 2, 3
> replacing SFPs 1, 2
> reset button
> resetting modules
> Restriction of Hazardous Substances (RoHS) Directive, recycling equipment
> Return Materials Authorization
> returning product
> RJ-45 connector 1, 2
> RMA (Return Materials Authorization)
> RoHS (Restriction of Hazardous Substances) Directive, recycling equipment
> RS-232 port 1, 2, 3, 4, 5

S

> safety
>   agency certification 1, 2
>   guidelines
> self-testing, modules
> serial numbers, locating
> SFM (switch fabric module) 1, 2
>   installing
>   removing
>   switch fabric slice
> SFPs (small form-factor pluggable transceivers) 1, 2
>   installing
>   removing
>   storing
> show interface command
> show version command 1, 2, 3, 4, 5, 6, 7
> single-bit errors
> site planning
> size
>   of E120 router
>   of E320 router
>   of rack
> slices, fabric
> slot combinations 1, 2
> slot disable command
> slot groups 1
>   overloading
> slot numbering 1, 2
> small form-factor pluggable transceivers
> SNMP for management access 1, 2
> space requirements 1, 2, 3, 4
> specifications
>   airflow 1, 2
>   dimensions 1, 2
>   distribution rack
>   electrical 1, 2
>   heat dissipation 1, 2
>   space 1, 2
>   weight 1, 2
> SRP (switch route processor) module 1, 2
>   errors on
>   installing
>   IOA
>   PCMCIA slot
>   powering down
>   redundancy
>   removing 1, 2
>   switch fabric slice 1, 2
> SRP IOA 1
>   cabling 1, 2
>   installing
>   removing
> starting router
> static electricity, protecting against
> storing, modules and components
> support, technical See technical support
> switch fabric modules
> switch fabric slices 1, 2
> switch router processor modules
> switches, power 1, 2
> switchover, SRP modules
> synchronization, SRP modules
> system maintenance

T

> technical support 1
>   contacting JTAC
> Telnet connection to router
> temperature
>   excessive 1, 2
>   monitoring
>   requirements 1, 2
> text and syntax conventions
> thermal protection mode 1, 2, 3
> timing port
> tools required
>   cabling router
>   installing modules
>   removing components 1, 2
>   unpacking router
> troubleshooting 1, 2
>   booting
>   cables 1, 2
>   clocking
>   double-bit errors
>   Ethernet link
>   fans 1, 2
>   LED activity for
>   modules 1, 2
>   power failure 1, 2
>   safety guidelines

U

> uninstalling modules
> unpacking router
> upgrading NVS cards

V

> ventilation

W

> Waste Electrical and Electronic Equipment (WEEE) Directive. See WEEE Directive
> WEEE (Waste Electrical and Electronic Equipment) Directive, recycling equipment
> weight
>   of E120 router
>   of E320 router
>   of rack 1, 2