Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# t1 fdl string

#### Syntax

t1 channel fdl string { eic eicValue | fic ficValue | lic licValue | unit unitValue |
pfi pfiValue | port portValue | generator generatorValue }

no t1 channel fdl string { eic | fic | lic | unit | pfi | port | generator }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Defines an FDL message on a T1 channel on a CT3 interface as defined in the ANSI T1.403 specification. Currently, FDL strings can be configured only locally. The no version restores the default value to the specified FDL message or to all FDL messages.

#### Options

- channel—One or more individual T1 channels, ranges of T1 channels, or combination of individual channels and ranges, in the range 1–28 (no spaces); for example, 3,7-15,19-13,27
- eicValue—Equipment identification code; 1–10 characters; default value is the null value
- ficValue—Frame identification code; 1–10 characters; default value is the null value
- licValue—Line identification code; 1–10 characters; default value is the null value
- unitValue—Unit identification code; 1–6 characters; default value is the null value.
- pfiValue—Facility identification code to send in the FDL path message; 1–38 characters; default value is the null value.
- portValue—Equipment port number to send in the FDL idle signal message; 1–38 characters; default value is the null value.
- generatorValue—Generator number to send in the FDL test signal message; 1–38 characters; default value is the null value.

#### Mode

Controller Configuration

#### Published: 2011-10-04

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out