Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- ?????? - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- ?? - China
- India
- ?? - Japan
- ???? - Korea
- ?? - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

# Rate-Limit Profile Management on E Series Broadband Services Routers, Release 12.3

Rate-limit profiles are a set of bandwidth attributes and associated actions. This page provides information about the JunosE Software features that you can use to configure rate-limit profiles on E Series routers.

JunosE Software Documentation for E Series Broadband Services Routers, Release 12.3

- Overview
- Configuration
- Administration
- Troubleshooting

How Rate-Limit Profiles Work
Rate Limits for Interfaces Overview Hierarchical Rate Limits Overview Percent-Based Rates for Rate-Limit Profiles Overview One-Rate Rate-Limit Profiles Overview Two-Rate Rate-Limits Overview Bandwidth Management Overview

Configuration Tasks for Rate-Limit Profile Management
Creating Rate-Limit Profiles Policy Parameter Quick Configuration Setting the Committed Action for a Rate-Limit Profile Setting the Committed Burst for a Rate-Limit Profile Setting the Committed Rate for a Rate-Limit Profile Setting the Conformed Action for a Rate-Limit Profile Setting the Exceeded Action for a Rate-Limit Profile Setting the Excess Burst for a Rate-Limit Profile Setting the Mask Value for MPLS Rate-Limit Profiles Setting the Mask Value for IP and IPv6 Rate-Limit Profiles Setting the Peak Rate for Rate-Limit Profiles Rate-Limiting Traffic Flows
Configuration Tasks for One-Rate Rate-Limit Profile Management
Creating a One-Rate Rate-Limit Profile Configuring a TCP-Friendly One-Rate Rate-Limit Profile Setting a One-Rate Rate-Limit Profile
Configuration Tasks for Two-Rate Rate-Limit Profile Management
Creating a Two-Rate Rate-Limit Profile Setting the Peak Burst for Two-Rate Rate-Limit Profiles Setting a Two-Rate Rate-Limit-Profile

Monitoring Tasks
Monitoring Rate-Limit Profiles Monitoring Control Plane Policer Information

Knowledge Base
http://kb.juniper.net/

## Downloads

- Policy Management Configuration Guide, Release 12.3.0
- Rate-Limit Profile Management on E Series Broadband Services Routers

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out